# COMPARATIVE ANALYSIS OF THE SPATIAL AND TEMPORAL VARIATIONS IN HYDROLOGICAL PARAMETERS AT KAINJI AND SHIRORO DAMS, NIGER STATE, NIGERIA

**By**

# ABUBAKAR, Fatimah MTech/SPS/2016/6582

**DEPARTMENT OF GEOGRAPHY FEDERAL UNIVERSITY OF TECHNOLOGY, MINNA**

# OCTOBER, 2019

**ABSTRACT**

Climate variability has been one of the major issues of the 21st century. The idea is to understand the differences in the climatic conditions and long-term catchment regimes using mean monthly seasonality indices and to explore the differences in the hydrological parameters at the long-term event scale. This comparatively analyze of spatial temporal variations in hydrological parameters at Kainji and Shiroro Dams in Niger State towards achieving a better future plan in the area. Quantitative and qualitative research approach was used, geospatial techniques were used to analysis the landuse pattern of the dams areas. Landsat satellite imagery was also acquired for 1997 to 2017. The imagery was subjected to digital process and five landuse classes were generated. Mann-Kendall test and Sen’s slope test on the monthly coefficient of variation for rainfall, reservoir inflow, reservoir elevation. The results show rainfall deviations increased between 1998 and 1999. On decadal basis, the years 1998, 1999, 2004, and 2006 have positive rainfall deviations while the remaining years have negative and least rainfall deviations. It was also revealing that evaporation deviation was increased in the years 1995 but it reduced drastically between 1993 and 1994. The analyses revealed a negative trend, and a slight decrease in rainfall and it can be brought to conclusion that since evaporation and reservoir inflow has the greatest impact because increase evaporation will increase and there will be shortage of water in the dam. It recommended that operators optimize the release of water from Kainji dam and ensure continuous monitoring of changes in hydro metrological variables to provide early warning for effective performance of the dam and to protect the environment.

|  |  |  |
| --- | --- | --- |
|  | **TABLE OF CONTENTS** |  |
| **Contents** |  | **Page** |
| Cover Page |  | i |
| Tittle Page |  | ii |
| Declaration |  | iii |
| Certification |  | iv |
| Dedication |  | v |
| Acknowledgement |  | vi |
| Abstract |  | vii |
| Table of Contents |  | viii |
| List of Tables |  | xii |
| List of Figures |  | xiii |
| **CHAPTER ONE** |  |  |

* 1. [INTRODUCTION 1](#_TOC_250038)
  2. [Background to the study 1](#_TOC_250037)
  3. [Statement of the Research Problem 4](#_TOC_250036)
  4. [Aim and Objectives of the Study 6](#_TOC_250035)
  5. [Research Questions 6](#_TOC_250034)
  6. [Justification of the Study 6](#_TOC_250033)
  7. [Scope of the study 6](#_TOC_250032)
  8. [The Study Area 8](#_TOC_250031)
     1. [Location of the study 8](#_TOC_250030)
     2. [Vegetation and soil of the study area 10](#_TOC_250029)
     3. [Climate of the study area 10](#_TOC_250028)
     4. [Hydrology of the area 11](#_TOC_250027)

[CHAPTER TWO](#_TOC_250026)

* 1. [LITERATURE REVIEW 13](#_TOC_250025)
  2. [Conceptual Framework on Hydrological Parameters in Dam 13](#_TOC_250024)
     1. [Concept of climate change 13](#_TOC_250023)
     2. [Impact of climate change on hydrology 15](#_TOC_250022)
     3. [Uncertainty in climate change predictions 16](#_TOC_250021)
     4. [Regional and seasonal variability in predicted climate 16](#_TOC_250020)

[2.1.5. Global hydrological cycle 17](#_TOC_250019)

* 1. [Theoretical Framework of Climate Change on Hydrological Parameters 20](#_TOC_250018)
     1. [Global climate scenarios 21](#_TOC_250017)
     2. [Scientific theoretical aspects 23](#_TOC_250016)
     3. [The hydrological concept 23](#_TOC_250015)
     4. The future change 25
     5. Global impact of climate change on the hydrologic cycle 26
        1. Impact on rainfall 26
        2. Impact on groundwater 27
        3. Impact on evapotranspiration 27
     6. Global temporal and spatial variations in water Storage 28
     7. Temporal and spatial variations of river discharge 28
     8. Spatial and temporal variability of rainfall 29
     9. Impact of climate change on water resources in Nigerian perspective 30
     10. Historical perspective of global climate variability 33
     11. Spatial and temporal variations for dam hydrological variables 33
     12. Impact of climate change on dam system in Nigeria 35
  2. Empirical studies of Spatial and Temporal Variability for Rainfall

and Temperature in Nigeria 35

CAHPTER THREE

* 1. [Materials and Methods 41](#_TOC_250014)
  2. [Type of Data Used 41](#_TOC_250013)
  3. [Methods of Data Analysis 42](#_TOC_250012)
     1. [Spatial-temporal characteristics of the dams 42](#_TOC_250011)
     2. [Comparative analysis of the spatial-temporal characteristics of the dams 42](#_TOC_250010)
     3. [Spatial variations of rainfall, reservoir inflow, reservoir elevation, evaporation and turbine discharge in Shiroro and Kainji dams 43](#_TOC_250009)
     4. Comparative analysis of the spatial variations on discharge as a function

of human activities 45

[CHAPTER FOUR 46](#_TOC_250008)

* 1. RESULT AND DISCUSSIONS 46
  2. Spatial variations of rainfall, reservoir inflow, reservoir elevation, evaporation and turbine discharge in Kainji 46
  3. Comparative analysis of the Spatial-temporal characteristics of the dams 50
  4. Spatial variations of rainfall, reservoir inflow, reservoir elevation, evaporation and turbine discharge in Kainji 52
     1. [Trend analysis of rainfall 52](#_TOC_250007)
     2. [Trend analysis of evaporation 56](#_TOC_250006)
     3. [Trend analysis on reservoir inflow 59](#_TOC_250005)
  5. Spatial variations of rainfall, reservoir inflow, reservoir elevation, evaporation and turbine discharge in Shiroro 64
     1. Spatial Variation of Rainfall in Shiroro 64
     2. [Trend analysis of Evaporation in Shiroro 67](#_TOC_250004)

[CHAPTER FIVE 75](#_TOC_250003)

CONCLUSION AND RECONMENDATIONS 75

* 1. [Conclusion 75](#_TOC_250002)
  2. [Recommendations 76](#_TOC_250001)

[REFERENCES 77](#_TOC_250000)

APPENDIX 81

|  |  |  |
| --- | --- | --- |
|  | **LIST OF TABLES** |  |
| **Table** |  | **Page** |
| 4.1 | Summary of Kainji Landuse Classification 1997-2017 | 48 |
| 4.2 | Summary of Shiroro Landuse Classification 1997-2017 | 50 |
| 4.3 | Trend analysis of rainfall between 1987 and 2017 using Mann Kendall test | 55 |
| 4.4 | Trend analysis of evaporation between 1987 and 2017 | 57 |
| 4.5 | Trend analysis of reservoir inflow between 1987 and 2017 | 59 |
| 4.6 | Mean Monthly Rainfall and Evaporation at Shiroro dam | 66 |

# LIST OF FIGURES

**Figures**

# Pages

* 1. Study area map 9
  2. Hydrological map of Kainji 11
  3. Hydrological Map of Shiroro 12
  4. Climate Change defining 14
  5. Different aspect in hydrological impact analysis 15
  6. Global hydrological cycle 18
  7. Hydrological components on a catchment 19
  8. Hydrological Model 25
  9. Causes of climate change 31
  10. Relationship between climate change and water resources 32
  11. Kainji Landuse Classification of 1997, 2007 and 2018 47
  12. Shiroro Landuse Classification of 1997, 2007 and 2018 49
  13. Kainji NDVI analysis between 1997, 2007 and 2017 51
  14. Shiroro NDVI analysis between 1997, 2007 and 2017 51
  15. Mean Monthly Rainfall of Kanji 52
  16. Rainfall deviation 54
  17. Mean Monthly Evaporation in Kianji Dam 56
  18. Evaporation deviation 58
  19. Mean Monthly Reservioir inflow in Kainji 60

**CHAPTER ONE**

# INTRODUCTION

# Background to the Study

Hydrology is the science of water which deals with the water of earth and its atmosphere. It is the study of occurrence, circulation, distribution, chemical and physical properties of all forms of water and also their reaction with the nature including human (Apalando, 2012). It is an important aspect for the living being including both human and the environment. It concerns with the water in streams, lakes, rainfall, snowfall, snow, ice on the land and even water occurring below the earth’s surface in the pores of the soil and rocks. Hydrological parameters such as precipitation, surface runoff, evapotranspiration, interception, infiltration, change in soil moisture, river flow, and change in groundwater storage are part of Earth's dynamic ecosystem.

Climate and human induced changes on catchment hydrological processes are major concerns for scientists, water decision-makers, and politicians. Different scenarios of climate change and its impact on water balance directly and on ecological, chemical, and geomorphological processes indirectly are the main issues of many studies in the last ten years all over the world. Most of them were dealing with different climate scenarios and their impact on global ecosystem, water management, or economy. Global modelling with simulating global water cycle and in that context analysing hydrological extremes and water balance components is the most common approach, as Corzo Perez *et al*. (2011) stated (Corzo-Perez *et al.*, 2011). Droughts are global hydrological phenomena found to increase in duration, area, and severity, according to Lloyd-Hughes *et al*. (2013). But validation of global models had to be done by observations on smaller scale, on the number of catchment areas of different characteristics, as it was studied by Stahl *et al*. (2010).

Climate change is the alteration in the temperature, rainfall, humidity, wind and seasons. It is the seasonal alteration of weather over an extended period due to global warming (Apalando, 2012). These alterations have an impact on surface water like a dam, rivers, agriculture production, and causes either flood or drought in the area. Globally, the effect of climate change has led to numerous issues in water resources like flooding and drought (Shen and Qiang, 2014). Rainfall is the only parameter that changes the reservoir inflow, reservoir elevation and turbine discharge in the dam (Shen and Qiang, 2014). These changes occur in space and time. Rainfall inconsistency in different locations over time causes counterpart runoff generation which affects water availability positively or negatively in the area (Warwade *et al*., 2018). The rate of change of runoff has a critical effect on hydrological cycles and its variables. Runoff influenced by human activities such as land use and housing development at the upstream and climate change. Identification of the spatial and temporal variations caused by rainfall and runoff is essential for water resources planning and management (Lee and Kim, 2017).

Climate variability has been one of the major issues of the 21st century. In fact, its importance keeps on increasing with the realization that its impacts cut across all sectors of a country’s economy. Hence it should not only be looked at just as an environmental issue but also a developmental issue. Presently the scientific consensus on climate change is that human activity is very likely the cause for the increase in global average temperatures over the past several decades (IPCC, 2001). The increase in the world’s population over the last century, complemented by the rise in the standards of living, has resulted in a rise in the demand for energy. According to John and James (2011); Adegbehin, *et al.,* (2016) Scientists predict that the global population will swell to over 10 billion by 2050. The impacts of climate variability and change are real and would continue to affect sensitive sectors of the global economy. Productive sectors such as

agriculture, water, health, energy, and transport among others bear the brunt of these variability and change in the world’s climate. Even though the entire globe will experience the impacts of these changes, the more severe impacts will be felt in low latitude developing countries where several non-climatic stressors are already at play (IPCC, 2007a). Sub-Saharan Africa continues to exhibit vulnerability to variability and change in climatic parameters such as temperature, rainfall and extreme events resulting from both anthropogenic climate change and natural variability. The principal known source of tropical climate variability is the El Niño-Southern Oscillation [ENSO] (Collins *et al.,* 2010; Camberlin *et al*., 2001).

The Intergovernmental Panel on Climate Change (2007) reported that rainfall variability on spatial and temporal had increased globally. These variations affect dam variables such as reservoir elevation, reservoir inflow, and turbine discharge. Furthermore, the disposition of spatial and temporal rainfall variability and others hydrological variables such as reservoir inflow, reservoir elevation, and turbine discharge were poorly understood (Cristiano *et al,* 2017).

The spatial temporal variations of hydrological characteristics are one of the key factors controlling the development and stability of natural ecosystems. From a hydrological perspective, spatial temporal analysis of runoff and precipitation is an appealing method for inferring flood generation mechanisms, which, in turn, supports other hydrological applications, such as hydrological regionalisation. Recently, the assessment of hydrological seasonality and regime stability has attracted a renewed interest, especially in connection with water resources management, engineering design and land cover and climate change assessment studies (Krasovskaia and Gottschalk, 2002; Krasovskaia *et al*., 2003; Bower *et al*., 2004; García and Mechoso, 2005).

Although, previous studies use weather radar to analyse the spatial and temporal variation and the outcome was poorly understood. Presently, numerous studies use multivariate statistics such as cluster, discriminant and Principal component analysis and Mann Kendall test to analyse the spatial and temporal variation of hydrological variables. Shen and Qiang (2014) examined the spatial and temporal variation of annual precipitation in a river of the loess plateau in China and multivariate statistical methods, and Mann Kendall were used. Their results showed that there was two spatial pattern that increases in the northwest, a decrease in the southeast and an increase in the west and the decrease in the east. Javari (2016) examined the spatial-temporal variability of seasonal precipitation in Iran. This study used an annual time series procedure and spatial (GIS) method, and their results showed that the rainfall had two spatial patterns in the area.

Hence, this study will comparatively analysis the spatial temporal of hydrological parameters of both Kainji and Shiroro dam within the context of ecosystem sustainability. The main idea is to understand the differences in the climatic conditions and long-term catchment regimes using mean monthly seasonality indices, and to explore the differences in the hydrological parameters at the long-term event scale. It is anticipated that the combination of both concepts within the framework of comparative hydrology may give an insight into the main hydrological processes in Kainji and Shiroro dams. The two hydrological dams have many common features with respect to runoff forcing and generation. Similar precipitation regimes exist in both areas (Tolulope, 2011).

# Statement of the Research Problem

The overdependence on hydropower has exposed the country to the impacts of climate variability. One of the potential effects of variability in climate, especially reduction in the amount and deviation in the distribution of rainfall, is the possibility of changes to

river flow and runoff which will affect energy supply from hydropower sources (Energy Commission & United Nations, 2012) Harrison *et al*., (2014). The existing hydropower capacity in Nigeria was built long before engineering and general public were aware of the impact of climate change on large infrastructure. Sudden climate variability has posed a dangerous threat in our poorly managed hydropower dam. Rising global temperatures will lead to an intensification of the hydrological cycle, resulting in drier dry seasons and wetter rainy seasons, and subsequently height and risks of more extreme and frequent floods. It will equally have significant impact on the availability and accessibility of water as well as the quantity of water that is available and accessible. All these factors highlighted will have an adverse impact on our hydropower dams. Therefore, periodic check on hydro climatic condition of our various dams is of serious concern, because failure of it will result to economic loss, and its attendant problems.

This study is purposely undertaken due to the frequent destruction of vegetation, farmlands and residential area downstream of Kainji and Shiroro dam. Biophysical impact analysis is necessary in order to reduce the impact of subsequent flooding event in the community. Government, although had already conducted many surveys to measure and assess flood damage, but the impact assessment at the micro-level based on community data, including the effect on the community hasn’t been done yet. No such studies attempted to link these destructions to emission of greenhouse gases whose increase in the negative environmental consequences of dam construction on inundation of terrestrial habitats, modification of hydrological regimes, and modification of aquatic habitats is thus, emphasized lead to climate change. Therefore, this study will be carried out to comparatively analysis the spatial and temporal variations in hydrological parameters of Kainji and Shiroro Dams in Niger State for effective sustainability of ecosystem.

# Aim and Objectives of the Study

The aim of the study is to comparatively analyze the spatial and temporal variations in hydrological parameters at Kainji and Shiroro Dams in Niger State towards achieving a better future plan in the area. The specific objectives are to:

* + 1. examine the spatial-temporal characteristics of Kainji and Shiroro Dam;
    2. examine the spatial variations of rainfall, reservoir inflow, reservoir elevation, evaporation and turbine discharge in Shiroro and Kainji dam.
    3. compare the spatial variations on discharge as a function of human activities, climate change and land use patterns in the upstream areas of the selected dams

# Research Questions

* + 1. What is the spatial-temporal characteristics of Kainji and Shiroro Dam;
    2. What are the spatial variations of rainfall, reservoir inflow, reservoir elevation, evaporation and turbine discharge in Shiroro and Kainji dam?
    3. Are there difference in spatial variations on discharge as a function of human activities, climate change and land use patterns in the upstream areas of the selected dams

# Justification of the Study

The spatial and temporal distribution of hydrological variables such as rainfall, reservoir inflow, reservoir elevation and discharge are crucial in hydrology, water resource management, agriculture and irrigation under climate change. The noesis of the spatial and temporal variation of the reservoir inflow, reservoir elevation, and turbine discharge is essential for water resources planning and management. The knowledge of spatial and temporal changes of reservoir inflow, reservoir elevation, and turbine discharge will be used as an essential tool for quantifying the variations (Saraiva *et al*., 2015) and predicting

future hydrological variables like reservoir inflow, reservoir elevation and turbine discharge under rainfall variability and climate change.

The significance of this research cannot be over emphasized, especially for the optimum result in saving lives and protection of properties in the long run. In the past, the spatial temporal of hydrological characteristics was analysed mainly in the context of flooding (Falkenmark & Chapman, 1989). The main idea was to study the character of hydrological processes and to identify regions with similar hydrological responses. There are numerous studies on the spatial temporal variations of the long-term mean monthly runoff regime (e.g. Lvovich, 1938; Pardé, 1947; Gottschalk, 1985; Haines *et al.*, 1988; Arnell *et al*., 1993; Krasovskaia *et al.*, 1994; Dettinger & Diaz, 2000; Bower *et al*., 2004; Johnston & Shmagin, 2008). In many studies the hydrological regime is analysed over a single region (Pfaundler, 2001; Archer, 2003; Birsan *et al*., 2005; Assani *et al*., 2006; Molnar & Burlando, 2008; Petrow *et al*., 2007; Sauquet *et al.*, 2008; Solin, 2008), but only a few studies compare two dams with large data sets to evaluate the seasonality across the boundaries of administrative units (Krasovskaia, 1995, 1996; Dettinger & Diaz, 2000; Krasovskaia & Gottschalk, 2002). Therefore, this study will fill the gap by comparatively analysis two big dam (Kainji and Shiroro) in the context of their spatial temporal characteristics in hydrological parameters.

This study requires an understanding of the hydrological characteristics and its interaction with the spatial temporal variations of the catchment. Hence, for effective planning and application of water resources management, there should be a basis or a study that must expose the areas that need attention. In this regard, this study will provide the opportunity for well-structured spatial and temporal variation of hydrological parameters and offer a sound scientific analysis for a coordinated management and planning. This in turn will facilitates reasonable and equitable use of scarce and vulnerable water resources by all

stakeholders. It is hoped that the results from this study will have significant implications on the current and future land and water resources management in Nigeria.

# Scope of the Study




The focal point of this study covers Kainji and Shiroro dams, the study deal with the hydrological parameters such as rainfall, reservoir inflow, reservoir elevation, evaporation and turban discharge, it will cover a duration of 30 years (1987-2017). It examine and compare the spatial variations of the hydrological characteristics of the area and also use geospatial techniques to analysis the landuse pattern of the dam’s areas.

# The Study Area

# Location of the study

Geographically, Shiroro dam is located on 6° 51’ 00” E and 6° 75’ 10’’ E longitude and

latitude 9° 58’ 00” N and 9° 65’ 25’’ N at 550 meters elevations downstream of the confluence of Kaduna River with river Dinya as its tributary in Shiroro Local Government Area of Niger State (Usman and Ifabiyi, 2012). Also, Kainji dam is located on Longitudes 04°36′ 48″E, 4° 34'3 .8 "E and latitudes 10° 11'45.71"N, 09° 5 ′ 45″N in Borgu Local Government Area of Niger State (Ehigiator *et al*., 2017) as shown in Figure 1.1 and 1.2 respectively.



# Figure 1.1: Niger State showing Kainji and Shiroro Dams Source: Modified by Ministry of Land and Housing, Minna (2019)

# Vegetation and soil of the study area

Shiroro watershed is a guinea savanna which consists of coarse grasses, shrubs and woodland (Ovie and Adeniji, 1994). The watercourse, in most areas, is characterised by

evergreen short-bowled, broad-leaved trees (Ovie and Adeniji, 1994). Adegbehin *et al*., (2016) reported that vegetation in the areas consists of a mixture of grass, woodlands in Kainji. These are in the group of Northern Guinea savanna type. The soils in the area are sandy loam, loamy sand, and clay-loam to clay in the land bordering the river throughout the lake area. The river bedrock covered by a layer of coarse to the medium sand of variable thickness, fine sand and clay (Adegbehin *et al.,* 2016).

The soil parent material is derived from a number of geological formations. The precambricum crystalline and metamorphosed sedimentary rocks of the basement complexes, the upper cretaceous conglomerates, sandstones and silt-stones of the Nupe formation. The alluvium varying in texture from sandy to clayed odpleistocene to recent age. The various rock types may play a decisive role in the soil derived from them and determine to a large extent their physical and chemical properties. The soil type is alluvial. Soil types within the study area are well drained shallow to moderately deep. The color varies from very dark gravity brown to dark or strong brown or yellow red the name of the soil of the Shiroro catchment area are derived from pre-existing rock i.e. Precambrian basement (complex rocks) consisting of gross, granite amphibolies schist. The soil type is also further grouped from association which are named after important features such as towns and rocks which have been used after some scientist (Raltche 1973).

# Climate of the study area

The raining season occurred between the month April and October while the dry season came between November and March in both study area (Adegbehin *et al*., 2016). Kanji area has a daily maximum of 33.5oC in the warmest month while the mean annual temperature is about 30oC. The mean temperature in both seasons is 35oC (dry season) and 270C (raining season) in Shiroro area. The months of April and May are the hottest month while December and January are the coldest. (Kuti *et al,* 2015).

# Hydrology of the area

The variation in the reservoir water level is controlled by inflow into the lake (a) from the area surrounding the reservoir basin (white flood-August to November ); (b)from the upper catchment of the Niger (black flood- December to march)(2) rainfall at the lake about 1071mm,(3) evaporation losses of the water surface estimated at 1500-2000 mm (4)seepage (5)out flood through turbines for power generating purposes (6) spilling (manly to satisfy commitments downstream) (7)domestic water use and (8)irrigation water supply (Kuti, 2015). Figure 2.1 is the hydrological map of Kainji area.

o o

10 71 1 0 9 2

o



# Figure 1.2: Hydrological map of Kainji

o


10 92

# Source: Niger State Geographical Information System, 2019

Shiroro Lake was built on river kaduna, one of the principal tributaries of river Niger, its source is from plateau mountains and travels a distance of about 356km before emptying into reservoir. Unlike the most rivers in the Northern Nigeria, river Kaduna a perennial river. The river flow in a fairly straight course in the upper and middle stage within same

meaned at the lower course. Long profiles consist of a number of steep gradient valley steps which is separated by parches of others sit low gradient. Its course is interrupted where it cross hard rocks, deep gorges have been cut across the area of more pronounced steeps in the valley (Figure 1.3 Hydrological map of Shiroro). This includes the 5.0km ravine in the granite of Shiroro and the 9.5km gorge through schist of guria. Rainy season between April and October peak falls between August and September. Dry season spell usually between November and March. River Munya, SarkinPawa, Gum and Dinya are the major tributaries in the vicinity of the study area that feed the main Kaduna River (Kuti, 2015).

9o 35



9o 55

9o 35

# Figure 1.3: Hydrological Map of Shiroro

9o55

# Source: Niger State Geographical Information System, 2019

# CHAPTER TWO


# LITERATURE REVIEW

# Conceptual Framework on Hydrological Parameters in Dam

# Concept of climate change

Climate change refers to a change in climate that is attributed directly or indirectly to human activity that alter the composition of the global atmosphere and that is in addition to natural climate variability observed over comparable time periods. The intergovernmental panel on climate change has evolved its own usage of the term climate change as any change in climate over time whether due to natural variability or as a result of human activity. Attribution of climate change to natural forcing and human activities has been addressed by Working Group I of the IPCC in climate change 2001 which is the most recent assessment of research on the topic of climate change, (IPCC, 2001). The Working Group I report concludes that globally average surface air temperature is projected to warm 1.4 to 5.80C by the year 2100 relative to 1990, and globally averaged sea level is projected to rise 0.09 to 0.88m by the year 2100.

Climate change is a long-term change in the statistical distribution of weather patterns over periods of time that range from decades to millions of years. It may be a change in the average weather conditions or a change in the distribution of weather events with respect to an average, for example, greater or fewer extreme weather events. Climate change may be limited to a specific region, or may occur across the whole Earth. According to the National Oceanic and Atmospheric Administration (NOAA), there are 7 [indicators](http://www.noaanews.noaa.gov/stories2010/20100728_stateoftheclimate.html) that would be expected to increase in a warming world, and 3 indicators would be expected to decrease. In recent usage, especially in the context of environmental


policy, climate change usually refers to changes in modern climate. It may be qualified as anthropogenic climate change or anthropogenic global warming (AGW). Figure 2.1 shows 10 indicators of a human fingerprint on climate change.

# Figure 2.1: Climate change defining Source: Modified from John 2011

Climate change within Nigeria during the next 100 years will depend primarily on the global change in climate. In turn, expected global change in climate will depend on increase in the concentrations of the greenhouse gases including carbon dioxide, methane and, nitrous oxide. Increasing concentration of greenhouse gases in the atmosphere enhances the potential of the atmosphere to conserve heat and therefore bring about global warming.

# Impact of climate change on hydrology

Evaluating regional impacts from possible climate change in the future requires a methodology to estimate certain meteorological variables for the time period and the geographical region of interest. In general, two physical systems are involved: the climate system and the hydrological system (Figure 2.2). The effect of greenhouse gases emissions forcing on the climate system can be simulated by GCMs. Many impact analysis studies in the past were based merely on the results of such simulations. The results available at the time from GCM simulations were limited, and the impact analysis based on such data are the first attempts to evaluate impacts from climate change, as predicted by physical models of the atmospheric dynamics.



# Figure 2.2: Different aspects involved in hydrological impact analysis of climate change

**Source: Modified from GCM, 1997**

# Uncertainty in climate change predictions

There is wide acceptance that anthropogenic activity is leading to global changes in climate through increased concentrations of greenhouse gas (IPPC, 2001). Although there is general consensus that the climate in the UK is changing and that the rate of change is likely to be influenced by ongoing anthropogenic activity, it is not possible to predict with any certainty the likely future climate in the next 50-100 years. There remains substantial and possibly growing uncertainty of the most likely climate change outcome over the medium to long term (Jenkins and Lowe, 2003; Murphy *et al*., 2004). In particular, the uncertainties will preclude firm predictions. They stem from uncertainties over trends in emissions, uncertainties over the scientific understanding of the climatic processes involved, uncertainties about how these will disaggregate regionally and uncertainties generated by natural variability. Moreover, projected outcomes from equally probable futures diverge substantially in the longer term. Exemplifying these uncertainties, future model projections for the 2080s include: Global temperature over the next 100 years increasing by between 1.5 and 5.5°C; Summer mean temperatures for the UK increasing by 3°C to >8°C depending on location; Global mean precipitation increasing by between 2 and 7 per cent; • Winter precipitation for the UK increasing by 1-60 per cent and summer precipitation changing from less than –30 per cent to more than +4 per cent, depending on the models used;

# Regional and seasonal variability in predicted climate


Accepting the limitations to the predictive outcomes stated above, work to date in the UK indicates that there will be both regional and seasonal variability in the rate and influence of climate change. Having considered the caveats on the confidence that can be ascribed to using single CGM outputs to simulate potential future climate (Jenkins and Lowe, 2003), it is illuminating to consider the future climate outcomes that may be produced.

To frame a relatively severe potential outcome, the UKCIP02 medium–high emissions scenario has been used, projected to the 2050s, to provide an indication of the sensitivity of freshwater ecosystems vulnerable to climate change in this study. Relevant abiotic factors associated with climate are introduced are changes in rainfall, air temperature (as mean and diurnal range), humidity, wind speed and solar radiation (as cloud cover). These factors are all addressed by UKCIP (Hulme *et al.*, 2002), including regional and seasonal perspectives.

These modelling outputs provide a general indication of the potential regional and seasonal changes. This is reasonable for general shifts in ecological function, but the extremes may be more significant for habitat change and species distributions. The UKCIP02 scenarios provide a considerable amount of new information on future changes in daily climate, which is important for analysing possible changes in extreme events. These include the number of ‘extremely’ warm days, changes in number of ‘intense’ rainfall days, changes in precipitation for a range of return periods (2-20 years) and changes in daily mean wind speeds for a range of return periods (2-20 years).

# 2.1.5. Global hydrological cycle


The hydrological cycle refers to the repeating effect of different forms of water movement and changes of its physical state in nature on a given area of the Earth (Kuchment, 2004). Water movement in the hydrological cycle covers atmosphere, hydrosphere, lithosphere, and biosphere and strongly depends on the local peculiarities of these systems (Kuchment, 2004). The function of the phenomenon in hydrological and their description depend on the chosen spatial-temporal scales and the significant parts of the terrestrial hydrological cycle (Kuchment, 2004), and the global hydrological cycle as shown in Figure 2.3 and 2.4.



# Figure 2.3: Global hydrological cycle Source: Modified from Kuchment, 2004

The mean rainfall on the earth’s surface equals total global evaporation. Nevertheless, the complete annual evaporation from the ocean surface is higher than the rain. The excess evaporated water (about 47 000 cubic kilometres) is transported by air currents from the oceans to the continents (Kuchment, 2007). Forty (40) percent of the rainfall goes back to the oceans as river runoff or as direct groundwater discharge to the beaches while the other part re-evaporates and falls back to the land (Kuchment, 2007).

Water moves through physical processes like evapotranspiration, precipitation, infiltration and river runoff (Stagl *et al*., 2014). These cycles require energy such as heat transfer, solar radiation and gravitational potential energy to transfer water from one reservoir to another. During this phenomenon water changes either in liquid or vapour/ice (Stagl *et al*., 2014).



# Figure 2.4: Hydrological components on a catchment scale Source: Modified from Kuchment, 2004

Hydrological processes involve different spatial and temporal scales. Runoff generation in the river networks are the key parts of the terrestrial hydrological cycle. In other to assess the terrestrial hydrological cycle, it is useful to know the important factor like topographic, vegetation, geological and soil parameters which determine the generation of runoff. These conditions give an opportunity to represent the land surface heterogeneity. The following hydrological parameters may be temporal and spatial variations in hydrological cycle:

1. **Rainfall:** the source of water in the earth surface is the rainfall. It drives the hydrological cycle over the land surface and changes surface salinity (and temperature) over the ocean and affects its thermohaline circulation (Oki, 2006). Highly variable, and rainfall behaviour in time and space domain compared to other major hydrological fluxes mentioned below makes the observation of this quantity and the aggregation of the process complex and difficult (Oki, 2006).
2. **Evaporation:** it brings back water flow from the surface to the atmosphere which produces latent heat flux from the surface (Oki, 2006). Atmospheric and hydrological conditions estimate the quantity of evaporation. Oki (2006) reported that the evaporation condition separated as driven hydrology.
3. **Transpiration:** it is the evaporation of water through the stomata of leaves. It consists of two different features from evaporation from soil surfaces. The stomata resistance is associated with dryness of soil moisture and physiological conditions of the vegetation via stomata opening and closing. The root of each plant transfers water from the soil than evaporation from bare soil. Vegetation’s modify the surface energy and water balance by changing the surface albedo and by intercepting rainfall and evaporating this rainwater (Oki, 2006).
4. **Runoff:** it is a nonlinear and complex process. It brings backwater to the ocean that is transported in the vapour phase by atmospheric advection for inland. This runoff that moves into the ocean is relevant for the freshwater balance and the ocean salinity. Rivers transported sediment, chemicals, and soil nutrients from continents to seas. Without rivers, global hydrologic cycles on the earth will never close. Surface runoff could generate higher rainfall intensity which is greater than the infiltration rate of the soil over the wetland surface. Saturation at land surface can be formed mostly by topographic concentration mechanism along hill-slopes (Oki, 2006).

# Theoretical Framework of Climate Change on Hydrological Parameters

Elevated greenhouse concentration drives to increased atmospheric moisture variability due to increased surface warming. This, in turn, leads to an accelerated hydrological cycle and increased regional precipitation variability. Climatic moisture content dramatically increases because of the exponential relationship between temperature and moisture

overload (Goswami and Himesh, 2002). Because temperature becomes an essential application on sensitive hydrological parameters such as evaporation and potential evapotranspiration (Goswami and Himesh, 2002) and relative humidity (Goswami and Himesh, 2002). Global warming has serious impact on global and regional hydrological cycles, which in shift become critical indications for water resources, agriculture, economy and environment. Production of spatiotemporal variability of water resource on a long-term basis equal varying anthropogenic and environmental pressure need complex. Modelling tools, wherein, GCM models (deal with climate change and rainfall prediction) are linked with hydrological models (Goswami and Himesh, 2002).

# Global climate scenarios

Global climate models are numerical models that are fundamentally very similar to the atmospheric models used for everyday weather forecasting. These models assume a given initial state of the atmosphere and predict the future developments with the help of hydrodynamic and thermodynamic relationships (so-called primitive equations). While weather forecasts are typically made for the next 1–2 weeks in a limited region, climate models are run for hundreds of years and cover the whole Earth. To make these calculations within a reasonable time, both the temporal and spatial resolution of the calculations are considerably lower than in the forecast models, typically about 10 min and 3°. One effect of this is that some small-scale processes, such as local convection, cannot be simulated directly but only estimated through simplified relationships.

A fundamental difference between forecasting models and climate models is that while the former predict the weather at a specific time (e.g. Wednesday at. 18:00), the latter instead predict statistical properties (e.g. the average rainfall in August). This is possible because of the limitations of climate, which are governed by regional characteristics in for example solar radiation, atmospheric composition and land surface. These restrictions

allow a basically forecasting model to not derail when run in a continuous “climate mode” but continue to generate statistically realistic weather sequences. In a climate model, certain large-scale interactions are considered, e.g. those that occur between the atmosphere and oceans. These play little role in the short term perspective but an important role on seasonal scales and therefore the atmospheric model is usually combined with an ocean model.

Future climate scenarios are typically generated by starting the climate model in pre- industrial times (typically 1850), with a generalized initial state, and driving it to the present day with observed greenhouse gas concentrations. The model is then run into the future (typically until 2100), with certain assumptions about how the concentrations of greenhouse gases will change in the future. This change is linked to six major so-called emission scenarios, which in turn are based on different assumptions regarding the speed and scale of different aspects of global development (socio-economic, demographic, technological, ecological, etc.).

A number of global models (around 10–20) are being developed at the main international meteorological/climatological institutes. While all models are based on the same fundamental physical relations, there are differences in the precise description of the many climatic processes and relationships that must be included. This means that the models give different results, even for the same emission scenario. If one also takes into account the results of different emission scenarios there is a large spread in the results, which increases the further into the future we look. At the end of this century, the increase in global average temperatures in the results vary between about 1°C and 5ºC, compared to today’s temperature. (By comparison, the observed warming over the past century is about 0.8ºC).

# Scientific theoretical aspects

Hydrological impact studies are basically highly applied research that is not explicitly aimed at increasing the understanding of natural processes. Well-established models are used to generate results that make it possible for society to prepare for future hydrologic conditions. But there are also elements that touch upon basic research. As mentioned in previous chapters, climate model results must be adjusted before being applied in the hydrological model. This adjustment is based on a detailed analysis and quantification of the systematic errors in the climate model’s temperature and precipitation. These errors are fed back to the climate modellers who in turn interpret them in terms of process descriptions and deficiencies in these. The deviations form the basis for new hypotheses about how the physical processes work and can best be described. The exact mechanisms of the formation of clouds and precipitation, for example, are not completely known and they are difficult to study empirically in full scale. To compare the model results with observations, based on progressively refined hypotheses about the mechanisms, is therefore a useful and widespread hypothetical-deductive method in this context (Thurén, 2007).

# The hydrological concept

Hydrological science is a clear example of empirically-based logical positivism (Hacking, 1983). Hydrology is basically about how water flows through the natural land and this process cannot be observed in detail (at least not with today’s measuring instruments). You can pour water on the ground, then dig a cut surface and see how far the water moved and what routes it took. But this provides only a snapshot. You can bring your soil back to the lab, put it in a Plexiglas cylinder, pour on water and see what happens. But these are not natural conditions. These empirical difficulties, combined with the inherent and equally hard-to-observe irregularities of natural soil (stratification,


rocks, roots, holes from worms and moles, treasure chests, etc.), mean that we cannot accurately describe the pathways of water in natural soil on the small scale.

To make the process manageable, we broaden the perspective to a larger scale, the catchment scale. This is inherently a defined system that follows certain physical laws, especially that of mass balance. The basic empirical material consists of observations of both the water coming into the system, rainfall (and possibly inflow from the upstream catchment area, but we ignore that here) and the water disappearing from the system, i.e. the discharge in the outlet and evaporation from the catchment area. Now we can through a chain of hypotheses use these data to obtain an understanding of the total water flow through the soil in the catchment.

# The hydrological model

A hydrological model calibrated for the current climate conditions also works in a future climate.

That the hydrological concept itself would not apply in the future seems unlikely. However, there are uncertainties regarding the validity of the related process descriptions. One example is evaporation, which is central to describing water balances over time. In one type of description, they increased more than proportionally with temperature. This description works well for today’s conditions, but when applied to future climate scenarios the effect was that large lakes in a relatively short period of time evaporated away, which is unrealistic. Figure 2.5 is an hydrological model.



# Figure 2.5: Hydrological Model Source: Modified from Thurén, 2007

* + 1. **The future change**

Climate change is the most significant future change for hydrological processes. Besides the climate, hydrological processes depend on catchment characteristics. In rural areas, changes in these characteristics are generally unlikely to have a substantial impact. It is mostly about local shifts between different types of agricultural land, limited felling of trees, etc., which rarely affect the hydrological processes in a dramatic way. Noticeable effects would require large-scale and systematic changes in the countryside, such as extensive deforestation or shifts from cultivation of traditional crops to new types (for example energy crops). In urban areas, however, it may well be assumed that changes in the urban environment have a stronger impact than the climate change. This is due to the large hydrological difference between natural soil (slow infiltration) and impervious surface (rapid runoff) and the resulting differences in flow dynamics. For urban or peri- urban areas becoming condensed or further exploited, the changes in land use are likely

to impact the hydrology more than climate change. The opposite could also happen, with less dense cities with more green space.

Another aspect concerns the regulation of rivers, for hydropower production or general levelling. Regulation has a strong impact on the hydrology, and future changes can for various reasons be significant. Perhaps many more rivers than today will to be regulated, or perhaps a perfect energy source will be invented so that we no longer need to produce hydropower.

# Global impact of climate change on the hydrologic cycle

* + - 1. **Impact on rainfall**

Sohoulande *et al.,* (2016) reported that increasing heat is the primary physical expression of climate change on the terrestrial system. Numerous studies agreed that increased atmospheric moisture is a consequence of more oceanic evaporation due to the increase of sea surface temperature. Nevertheless, the effect of a change in climate on rainfall is experienced in different ways worldwide. Modification in the term of frequencies of rainfall events, prolonged dryness, decreases in the number of rainfall events, and an increase of extreme rainfall events. At the annual level, profound diversions of season onsets and demises experienced (Sohoulande *et al.,* 2016). The impacts of these disturbances (i.e., drifts in season onset and demise, alteration of precipitation patterns) are significant for the society. For instance, the change in rainfall pattern often causes an important agricultural loss regarding yield. Also, the persistence of low rainfall jeopardises the sustainability of groundwater resources, since it often utilised as an option to overcome the deficit of water supply (Sohoulande *et al.,* 2016). However, this option of using groundwater has resulted in depletion issues. Subsequently, more policies are aiming to regulate the pressure on groundwater across the globe (Sohoulande *et al.,* 2016).

# Impact of groundwater

Water quality, quantity, and functionality are the parameters used to assess the impact on groundwater system (Sohoulande *et al.,* 2016). Naturally, streamflow sustained by groundwater, and it plays a critical role in hydrology. During the dry season, groundwater is the major water supplier of streamflow and river. Apart from raining season, the balance of the streamflow/river and base-flow controls the streamflow behaviour (Sohoulande *et al.,* 2016). An unbalanced situation often results in low-flow regime and impairments. Besides, groundwater recharge is controlled itself by soil infiltration, land- cover, and amount of rainfall. Under climate change, the disturbances in the rainfall regime coupled with land-cover degradation significantly change groundwater recharge (Sohoulande *et al.,* 2016). Water supply becomes problematic for streams if groundwater could not recharge adequately, and this scenario is more drastic when groundwater directly pumped for irrigation, domestic and industrial use. The use of groundwater has become an option for compensating for water deficit. However, this alternative raises important environmental and social concerns.

# Impact of evapotranspiration

Evaporation and transpiration are the important part of the water cycle. It depends on the magnitude of the terrestrial biophysical functionality (Sohoulande *et al.,* 2016). The amount of water involved in this phenomenon is a determinant of the local climate. Indeed, the long-term balance between evapotranspiration and rainfall controls the gradient of aridity and land-cover features (Sohoulande *et al.,* 2015). The rise of global temperature affects the atmospheric water demand under climate change directly. Finally, the actual moisture release in the atmosphere is higher than normal. The water vapour in the atmosphere results from the pressure exerted on soil moisture, water bodies, and plant

transpiration. Sohoulande *et al.,* (2016) reported that the trend of dryness is remarkable across the globe.

# Global temporal and spatial variations in water Storage

Guntner *et al*. (2007) reported that water storage acts important function in the water Earth’s, energy, and biogeochemical cycles. Water storage appends evaporative demand of plants. It serves for human consumption, including various types of agricultural and industrial use (Guntner *et al*., 2007). Water storage includes water on groundwater, vegetation surfaces, unsaturated soil or rock zone, surface water in rivers, wetlands, natural lakes, and human-made reservoirs. It estimated as the sum of soil moisture, groundwater, and surface water storage. Temporal storage variations were analysed at monthly, seasonal, and interannual timescales (Guntner *et al.,* 2007). An Empirical Orthogonal Function (EOF) is normally used to analyse the spatial variation in water storage. This multivariate technique is employed to identify the dominant simultaneous patterns of space-time variability (Guntner *et al*., 2007). A spectral analysis of the amplitude (principal component) of the EOFs was carried out to derive the preferred frequencies of storage variations (Guntner *et al*., 2007). Furthermore, the spatial continuity of water storage patterns depicted and spatial autocorrelograms estimated on a monthly basis. The gap in this work is that the temporal and spatial variations of water storage are presently not known with sufficient accuracy for large areas.

# Temporal and spatial variations of river discharge

Warwade *et al*. (2018) reported that the uneven distribution of rainfall leads to counterpart between water availability and demand so as irrigation structures be needed to redistribute water in line with the requirements of a specific region. The incidence of extreme rainfall events is relevant for the design of dams, spillways, flood protection structures, and drainage networks. The intensity of spatial, interseasonal, and inter-annual variability of

rainfall events have heightened risen in Asia over the past few decades (IPCC, 2014). Global, a rise in temperature of about 0.74℃ between 1906 and 2005 led to more considerable rainfall variability (Warwade *et al*., 2018). This phenomenon has a negative impact on crop water requirements, evapotranspiration, groundwater level depletion, environmental flows, trans-boundary issues, and interstate disputes, among others. Numerous works show that rainfall variability is increasing on both a spatial and a temporal basis. Various studies showed that the trend of India is strongly affected by atmospheric factors viz. regional pressure anomalies, sea surface temperature variations (Goswami *et al.* 2006), thereby making rainfall less predictable (Shiklomanov, 2007). Mann–Kendall (MK) test, Sen’s slope estimator, percentage change and breakpoint analysis are the methods for determination of the spatial and temporal variation of river discharge. Furthermore, identification of the downstream discharge trend is still a challenge for a large basin with sizeable spatial variation across the catchment, and a human factor which is affecting the hydrological cycle of the watershed.

# Spatial and temporal variability of rainfall

Globally, climate change is inducing severe issues. The difference in rainfall associated with runoff changes. This process has a negative impact on ecosystems and socioeconomic development (Shen and Qiang, 2014). There is an incessant natural disaster in Weihe basin. Hence, assessment of the spatial and temporal variation in rainfall in the pool is crucial for understanding changes in runoff, and a negative impact on the socioeconomic and ecological aspect of the region for developing robust, cost-effective strategies to adapt and mitigate the effects of climate change on hydrological variables (Shen and Qiang, 2014).


Rainfall is one of the prominent variables for qualifying water resources and understanding the climatic change impacts on the local hydrologic system in Haihe River

Basin (HRB) of China (Luo *et al.,* 2014). Inadequate knowledge of the variations of rainfall on time and space, systematical management of the reservoirs is not available, resulting in inefficient utilisation of water resources in the basin (Luo *et al.,* 2014). Therefore, the negative impact of the change in climate on the hydrologic cycle and water resources associated with considerable uncertainty (Luo *et al*., 2014).

The variability of the climatic variable is useful for identifying changes in variability patterns of the environment over time (Javari, 2016). Locally, in the recent periods, rainfall spatial-seasonal variability, temporal trends’ variability, and extreme consequences have caused massive damages to the environment (Javari, 2016). Therefore, numerous studies placed special emphasis on rainfall spatial-seasonal variability, temporal trends variability, and their impact on the environment. Globally, numerous analyses have examined spatial-seasonal variability and temporal trends’ variability at various temporal periods. The spatial and seasonal variability analysis method concentrated not only on estimating climatic variations but also demonstrating variations in a series of rainfall and other climatic elements (Javari, 2016). According to Cristiano (2017), inadequate information on spatial distribution of rain is a source of error in urban runoff estimation. Understanding of hydrological processes in urban areas is still poor especially in the interaction between rainfall and runoff (Cristiano, 2017). Rainfall event is classified and identified by looking at their variability in space and time. Spatial variability is defined as variability derived in multiple spatially distributed rainfall fields for a given point in time (Peleg *et al*., 2017). Peleg *et al*. (2017) also introduced the definition of climatologically variability as the variability obtained from multiple climate trajectories that produce different storm distributions and rainfall intensities in time.


# Impact of climate change on water resources in Nigerian perspective

Climate change is the variability in climate even if average weather conditions remain unchanged (Odjugo, 2010). Natural and artificial events cause changes in the environment. The primary physical factors that enhance climate change include volcanic eruptions and changes in the intensity of sunlight reaching the earth are the main factors of natural phenomena of climate (Odjugo, 2010). Figure 2.6 shows the detail causes of climate change.



# Figure 2.6: Causes of climate change Source: Modified from Odjugo, 2010

Nan *et al*. (2011) reported the relationship between water resources and the hydrologic cycle and linked to a change in climate. Water quantity variations is an indicator that change in environments such as rainfall and temperature variations affects water

resources, and achieved by the differences in hydrological cycle links (Nan *et al*., 2011). Globally, change in climate will cause the hydrologic cycle to redistribute water resources in time and space (i.e., spatial and temporal variations). This variations in water resources have a direct impact on the evaporation, runoff, soil humidity, etc. (Nan *et al*., 2011). Change in water resources and redistribution causes society and ecology to alter as well, and the water resources system variations will turn to affect the local climate (Nan *et al.,* 2011). The relationship between climate change and the hydrological cycle as shown in Figure 2.7.

# Figure 2.7: Relationship between climate change and water resources Source: Modified from Ifeanyi, 2011

In Nigeria, rainfall becomes more intense in the past 50 years and are projected to grow more frequent and severe (Ifeanyi, 2011). Alteration in climate is expected to cause

significant changes in yearly and seasonal rainfall and water flow, flooding (Ifeanyi, 2011).

# Historical perspective of global climate variability

The high-accuracy measurements of atmospheric CO2 concentration, initiated by Keeling in 1958, constitute the master time series documentation of the changing composition of the atmosphere (Le Treut, *et al,* 2007). These data have iconic status in climate change science as evidence of the effect of human activities on the chemical composition of the global atmosphere Keeling’s measurements on Mauna Loa in Hawaii provided a true measure of the global carbon cycle, an effectively continuous record of the burning of fossil fuel. They also maintain an accuracy and precision that allowed scientists to separate fossil fuel emissions from those due to the natural annual cycle of the biosphere, demonstrating a long-term change in the seasonal exchange of CO2 between the atmosphere, biosphere and ocean. Later observations of parallel trends in the atmospheric abundances of the CO2 isotope and molecular oxygen (O2) *(*Le Treut *et al, 2007)* uniquely identified this rise in CO2 with fossil fuel burning

# Spatial and temporal variations for dam hydrological variables

Temporal variation refers to a change of hydrological variables such as rainfall, reservoir inflow, reservoir elevation, turbine discharge with time. A spatial variation occurs when a quantity of hydrological variables such as rainfall, reservoir inflow, reservoir elevation, turbine discharge that measured at different spatial locations exhibits values that differ across the areas. Spatial variability can be assessed using descriptive spatial statistics such as the range.

Sakka (2011) reported that rainfall in the semi-arid and arid watershed qualified by a great unevenness of the small amount received in space and time. Approximately 80 per cent

of the annual rain collected during raining seasons for 3 to 6 months, and each rainfall event occurs with high intensity and short duration storms. Sakka (2011) reported that the particular features of the semiarid and arid hydrological processes include the marked seasonal variation in semiarid climates may require segregation of data by season. A combination of hydrological factors common in one season of the year may be virtually non-existent during another season. Besides, the particular combination of factors may exist for only a few days in several years and may render hydrological computation based on average values grossly erroneous. Actual evaporation from semi-arid zones is a highly transient phenomenon with extreme variation within a day because of the available water but not over a season. The temporary nature of evaporation also controlled by the rapid growth of vegetation to climax followed by rapid die-off (Sakka, 2011). In a humid climate, hydrological processes in the semiarid and arid region often vary significantly over different parts of a catchment (Sakka, 2011). Besides, the sparse vegetation cover and its sharp response to the first rain have an impact on the evaporation process prevailing in such regions. The rivers in such areas are generally characterised by having long periods of low flow regime (Sakka, 2011).

Another distinct characteristic of such regions is that in some cases infiltration could be minimal because of outcropped rocks on the slopes while it could be high in areas with fractured bedrock channels (Sakka, 2011). There could also be the possibility of channel infiltration from the bed of the rivers supplying the groundwater in the river downstream (Sami, 1992). This fact implies that especially during low flow regime the stream flow that originates from upstream will be depleted by the channel bed before it reaches the outlet (Sakka, 2011).

# Impact of climate change on dam system in Nigeria

Climate change is the variability in climate even if average weather conditions remain unchanged (Odjugo, 2010). Natural and artificial events cause changes in the environment. The primary physical factors that enhance climate change include volcanic eruptions and changes in the intensity of sunlight reaching the earth are the main factors of natural phenomena of climate (Odjugo, 2010).

# Empirical studies of Spatial and Temporal Variability for Rainfall and Temperature in Nigeria

Abaje *et al*. (2018) examined the spatiotemporal Analysis of rainfall distribution in Kaduna State linear trend line equation, second order polynomial, Cramer’s test, and student’s t-test. Abaje *et al*. (2018) reported that the result of the student’s t-test for the two nonoverlapping sub-periods (1961-1990 and 1991-2016) of each station showed that Kafanchan and Zaria were significantly wetter in the last 26 years (1991‒2016) while Kaduna had a healthy condition. Ifabiyi and Ashaolu (2015) assessed the spatiotemporal pattern of rainfall distribution over Ilorin Metropolis, Nigeria trend analysis using reduction analysis, and ordinary kriging with Gaussian semivariogram model; their results show that the variability and percentage change in the amount of rainfall over thirty (30) years. Besides, a spatial distribution of annual rainfall in Ilorin varied from one part to the other.

Ezemonye and Emeribe (2015) assess the spatial and temporal patterns of climatic change in the Sokoto-Rima River Basin, Sudano-Sahel region, Nigeria using Mann-Kendel, Spearman’s Rho, Linear regression, free distribution CUSUM, cumulative deviation and Worsley Likelihood tests. Their results show a decreasing trend in the time series of annual rainfall, while evidence of a rising trend detected in the time series of temperature.

Egor *et al.* (2015) examined the inter-annual variability of Rainfall in some States of Southern Nigeria using Standardized Anomaly Index, and the results showed that the variability in rainfall as Calabar, Port Harcourt, Owerri, and Enugu have 4062.70mm, 3911.70mm 3064.0mm and 2262.4mm. Besides, their least rain for these areas was 2099.4mm, 1816.4mm, 1228.4mm, and 913.10mm. Oguntunde *et al.* (2012) assessed spatial and temporal temperature trends in Nigeria, between 1901 and 2000 using Mann- Kendall test and spectral analysis, and their results showed that Annual temperature has risen by 0.03 oC/decade during the last century. Besides, alterations in minimum temperature are higher than that of maximum temperature. Their findings showed that yearly temperature showed significant negative correlation Southern Oscillation Index.

Akinsanola and Ogunjobi (2014) assessed rainfall and temperature variability over Nigeria using confidence levels, coefficients of kurtosis, skewness, and coefficient of variations, and their results showed that the longtime trends suggest a sequence of alternately decreasing and increasing trends in mean annual rainfall and air temperature in Nigeria.

Salami *et al;* (2011), worked on the assessment of climate variability on Kainji hydropower reservoir, Niger State Nigeria, they obtained the following rainfall data (2000-2009) reservoir inflow (1970-2003) and temperature data (1972-2009) from Kainji hydropower station. This study aimed to detect trends in the long-term hydro-climatic series using non-parametric methods. The annual and seasonal linear trends of rainfall, temperature, runoff, water level and evaporation were analyzed for stations in downstream Kaduna River Basin during 1975-2014. The non-parametric Mann-Kendall and Sen’s estimator of slope procedures were adopted to identify if there exists an increasing or decreasing trend with their statistical significance at 95% level of

confidence. The datasets were checked to account for auto-correlation prior to determining trends using Mann-Kendall test. The existence of abrupt changes was detected by means of Cumulative Sum Charts and Bootstrapping analysis. The results of study indicated increasing trends for seasonal and annual temperature and runoff series. Water level and evaporation revealed statistically decreasing trends both on annual and seasonal periods. However, for the period 1975 to 2014 no significant distinctive trend was observed for rainfall at the investigated stations. Change-points in time series were identified in all the investigated hydro-climatic records for the sub-basin. Generally, the detection of the trend for hydro-climatic variables by Mann-Kendall test conforms to Sen’s test results. It is concluded that the basin is sensitive to climate variability and water stress impacts which will affect food security. So, it would be necessary to make adjustments in the adaptive water-use strategies being adopted at present in the catchment.

Salami *et al.* (2010) worked on impacts of climate change on the water resources of Jebba hydropower reservoir. The meteorological and hydrological variables under study were subjected to statistical test. The study showed some notable changes in the climate of Jebba hydropower station, it reveals that for the past few years, rainfall and relative humidity have exhibited negative trends. This implies that both variables will decrease slightly, while for the past few years, the reservoir inflow, outflow and temperature have shown significant positive trends. This indicates that the parameters have tendency to increase and rate of their changes are significantly positive. The evaporation loss also shows negative trends and may be due to low relative humidity. The study concluded that there is positive impact of climate change on water resources of the study area due to increase in reservoir inflow and low evaporation, hence more water for hydropower generation.

Jimoh (2008) examined the operation of hydropower systems in Nigeria and observed that the combined installed capacity of power stations in Nigeria is far below the country’s electricity demand, resulting in epileptic supply of electricity. He noted that the situation is compounded by the failure of the existing power stations to operate at installed capacity and attributed the inability of the hydropower stations to operate at installed capacity to the following reasons.

1. Hydrological factors, such as seasonal deviation inflow to the reservoir, inter-annual deviation inflow to the reservoir with low and high extremes, conflict among competitive uses, and sediment trapped in the reservoir
2. Non-hydrological factors, such as maintenance and spare part problems, inadequate fund, human resources, and policy issues. The findings also revealed that the low and high extremes inter-annual deviation inflow to Kainji reservoir is caused by two distinct peaks at Kainji on River Niger. These are called black (December or January) and white (August or September) floods.

Daniel (2013) Climate Variability Impacts on Water Resources of the Area Kaduna was investigated in this report using 47years (1960-2006) record of hydro-meteorological data. The Climate variability was evaluated using a simple approach which considered variability as the difference between the means and standard deviations of climatic elements of two equal –length time periods. Other methods used include coefficient of deviation, time series methods and anomaly approach. The impacts of climate variability on water resources of the study area were investigated using comparative and correlation analyses. From the results, the hottest year within the zone was 1993 with day time temperature increase of15.3℃and a zonal average of 0.08℃, indicating warming while within the catchment, the highest increase in maximum temperature was 2.6℃.The

historical observations of temperatures, rainfall land evaporation in the study area indicated annual maximum temperature trend of0.12℃, annual minimum temperature trend of 0.88℃,annual mean temperature trend of 0.48℃, annual rainfall trend of 100mm and annual evaporation trend of 99mmwhich are all statistically significant except for the annual maximum temperature.

Jimoh and Ayodeji (2003) assessed the impact of the Gurara river inter basin water transfer scheme on the Kaduna River at the Shiroro dam, Niger state, Nigeria. The inter- basin water transfer 48 is intended to stabilize the Shiroro reservoir level. The paper examined the effect of the water transfer on the storage level of the reservoir, using fourteen years of daily inflow record to study the real time operation of the reservoir. The results indicated that with the water transfer, the reservoir attains its maximum operating level in July and maintains it until September or October, whereas the maximum operating level would have been attained in August without the transfer. Although the inter basin water transfer into the Shiroro reservoir would enhance power generation. But it will lead to increase flood frequency severity annually downstream of the dam. So, appropriate flood damage mitigation measures were recommended for the Kaduna River basin to optimize the benefit of the proposed interbasin water transfer scheme.

Garbrecht and Schneider (2008) worked on the impacts of decadal precipitation deviations on reservoir inflow, flood releases, and pool elevation in Fortcobb reservoir, at Central Oklahoma, using three dry periods and one wet period with the use of 1940- 2004 precipitation record. The study reveals that the differences in mean annual precipitation between dry and wet periods was 33% of the mean, and led to a corresponding 100% change in mean reservoir inflow, 170% change in mean annual flood releases from the reservoir, and a maximum pool elevation drop of 2 meter from the top

of the conservation pool. Thus, watershed runoff, reservoir inflow and flood releases were highly sensitive to decadal precipitation deviations. Yet, the only reservoir operation that appeared to be impacted by decadal precipitation deviations was the frequency of flood release activities. So it was observed that high reservoir inflows during wet periods led to an increase in flood releases. Also the increase in frequency of downstream flow was not believed to appreciably enhance stream habitat and riparian vegetation, due to the sporadic and intermittent nature of flood releases.

Keming and Bagale (2012) carried out a study on dam slope stability under the condition of rainfall. The study investigated the static and dynamic simulation analysis of the cracks using the strength reduction principle, to get the stress, strain and displacement distribution rule and the corresponding safety factor in the water level change and rainfall infiltration. It was observed that rainfall has a great influence on the slope stability of the dam. The rainfall impact causes change of the seepage and the stress field, influencing the stress and strain distribution of the dam, which will eventually change the situation of the dam skeleton and finally causing instability in the dam. The study shows that safety factor decreases along with rainfall duration increasing in the different return periods of rainfall. When the slope is reduced, slope safety factors reduce slowly in the range of allowable value.

# CHAPTER THREE

# MATERIALS AND METHODS

The study carry out a comparative analysis of spatial temporal variations in hydrological parameters at Kainji and Shiroro Dams in Niger State. It examine the spatial-temporal characteristics of the dams, compare the spatial-temporal characteristics of the Dams; examine the spatial variations of rainfall, reservoir inflow, reservoir elevation, evaporation and turbine discharge in Shiroro and Kainji dams and compare the spatial variations on discharge as a function of human activities, climate change and land use patterns in the upstream areas of the selected dams

# Type of Data Used

Three sets of data used in this study; namely: Climate, Hydrological and Remote sensing data sets. The climate data include annual rainfall and evaporation record of 30 years (1987-2017), hydrological record includes reservoir inflow, reservoir outflow reservoir elevation, and turbine discharge for 30 years (1987-2017) was collected from NIMET stations in Kainji and Shiroro dams. Landsat satellite imagery of the study areas (Kainji and Shiroro) was acquire from Ground Cover Land Facility (GFLF) for three decades (1987-2017). The imagery was use to examine the spatial-temporal characteristics of the landuse pattern in the study areas.

# Methods of Data Analysis

# Spatial-temporal characteristics of the dams

It involve the use of satellite imagery of the study area to analysis the spatial-temporal characteristics of the dam areas in terms of landuse surrounding Kainji and Shiroro the dam site. Landsat imagery of three decade (1987, 2007 and 2017) was used, the imagery was subjected to digital image processing, which basically involve classification of landuse surrounding the study area. Field reconnaissance survey and physical observations during the pre-satellite image analysis and use of GPS to capture geographical coordinates each community and coordinates for training site for accuracy assessment. In order to obtain the required information from satellite image data, processing and interpretation were made systematically. The interpretation phase preceded by establishing preliminary legend.

Basic for any landuse mapping is an appropriate classification scheme. This is required to organize the needed information in such a way that it would satisfy the research problem, objectives, type of resource data being sought and the physical nature of the terrain. When there is no prior land variance as the case of Nigeria, an appropriate one has to be developed. For the purpose of this study, a classification scheme suited to it will be developed. In this regard, a preliminary ground truth was carried out to serve as a guide. ArcGIS 10.1 was be used for image processing and classification and MS Excel was used for tables and graphical presentation of questionnaires analysis of the study.

# Comparative analysis of the spatial-temporal characteristics of the dams

Image thinning was carried out through contract. Contract generalized an image by reducing the number of rows and columns while simultaneously decreasing the cell resolution. The methods of analysis adopted in this are: Calculation of the area in hectares

of the resulting land use types for each study year was generated. Overlay operations. –

i.e. mathematical and logical operation between two raster layers on a pixel-to-pixel basis to detect change that has occur in the area, the images was overlay to detect the direction and extent of changes in the area.

The comparison of the spatial temporal characteristics use statistics assist in identifying the percentage change, trend and rate of change was determine. Percentage change to determine the trend of change can then be calculated by dividing observed change by sum of changes multiplied by 100.

(Trend) percentage change = observed change X 100

Sum of change 3.1

# Spatial variations of rainfall, reservoir inflow, reservoir elevation, evaporation and turbine discharge in Shiroro and Kainji dams

After establishing that these dams’ hydrological parameters are not serially autocorrelated, the study explore Mann-Kendall test and Sen’s slope test on the monthly coefficient of variation for rainfall, reservoir inflow, reservoir elevation, and turbine discharge. These tests was analysed in the Statistical software and data analysis add-on For Excel environment. The seasonal Mann-Kendall test takes proper account the seasonality of the time series which means that monthly data with seasonality of 12 months examine whether there is a trend in the overall series or not. The study explored Kendall tau statistic, τ, to test for randomness against the trend in hydroclimatic time series (Cigizoglu *et al*., 2005). In this test, the null hypothesis Ho states that the deseasonalized data (*x*1 *xn*) are a sample of *n* independent and identically distributed

random variables (Zhao *et al.,* 2017). The alternative hypothesis H1 of a two-sided test is that the distribution of 𝑥𝑘 and 𝑥𝑗 is not identical for all *k*, *j ≤ n* with *k* ≠ *j* (Zhao *et al.,*

2017). The test statistic (S) was calculated with equation 3.3 and 3.4, with mean zero and variance of S, computed by:

𝑉𝑎𝑟(𝑆) = [𝑛(𝑛 − 1)(2𝑛 + 5) − ∑𝑡 𝑡 (𝑡 − 1)(2𝑡 + 5)]/18 (3.2)

𝑆 = ∑𝑛−1 ∑𝑛

𝑆𝑔𝑛( 𝑥𝑗 − 𝑥𝑘) (3.3)

𝐾=1 𝑗=𝑘+1

+1 𝑖𝑓 (𝑥𝑗 − 𝑥𝑘)˃0

𝑆𝑔𝑛(𝑥𝑗 − 𝑥𝑘) = { 0 𝑖𝑓 (𝑥𝑗 − 𝑥𝑘) = 0

−1 𝑖𝑓 (𝑥𝑗 − 𝑥𝑘) = 0

(3.4)

and is asymptotically normal, where *t* is the extent of any given tie, and *t* denotes the summation over all relationship. For the cases in which *n* is more significant than 10, the standard variate Z computed by using the following equation (Cigizoglu *et al*., 2005):

𝑆−1

√𝑉𝑎𝑟(𝑆)

𝑖𝑓 𝑆 > 0

𝑍 = [{

𝑆+1

{𝑖𝑓 𝑆 = 0] (3.5)

√𝑉𝑎𝑟(𝑆)

𝑖𝑓 𝑆 < 0

The test statistic 𝑍𝑠 was used as a measure of the significance of the trend. In fact, this test statistic was also used to test the null hypothesis, 𝐻0: There is no monotonic trend in the data. If 𝑍𝑠 is greater than 𝑍𝖺 2, where represents the chosen significance level (usually 5%, with 𝑍0.025= 1.96), then the null hypothesis is invalid, meaning that the trend is significant. Besides, the calculated slope is multiplied by the number of years to indicate

the magnitude of change over the period (Oguntunde *et al.,* 2012). The objective one will achieve through the use of Mann-Kendall test to assess the trend of the temporal variations of the monthly coefficient of variation for rainfall, evaporation, reservoir inflow, reservoir elevation, and turbine discharge. These non-parametric test was used to achieve objective two.

# Comparative analysis of the spatial variations on discharge as a function of human activities




In order to achieve objective three, the monthly coefficient of variation (CV) for hydrological parameters between 1987 and 2017 at different locations was used for this study. Two-way analysis of variance with post-hoc comparison was used to compare spatial and temporal variations of the hydrological parameters of each dam. In spatial variations analysis, the variables were grouped as dependent variable (discharge) and independent variables such as monthly CV for rainfall, evaporation and locations with Shiroro dam as a control. In temporal variations analysis, the variables were grouped as dependent variable (discharge) and independent variables such as monthly CV for rainfall, evaporation and time (April to October) with months between 1980 and 2017 as control. The residual of the model was subjected to Durbin-Watson test (to determine whether the dataset is autocorrelated or not) and normality test. Also, these hydrological parameters was subjected to equality of variance (parametric test) and Kruskal-Wallis test (Non- parametric test). The outlier test was examined to check whether to reject null hypothesis or not.

# CHAPTER FOUR

* 1. **RESULTS AND DISCUSSION**

# Spatial-temporal characteristics of Kainji and Shiroro Dams

The result of spatial temporal characteristics of Kainji dam is presented in Table 4.1, the spatial temporal analysis is between 1997, 2007 and 2017. Figure 4.1 shows the spatial analysis of landuses and their changes in the area within the study period. Six landcover classification were generated from the analysis, Buit up area, Vegetation, Cultivated land, Bareland, Water body and weeds. It shows that in 1997 water body cover 22.12% of the total landcover Vegetation covers 44.15%, Cultivated land covered 23.42%, Built up 9.62%, weeds 0.56% while bare land covered a total of 0.13%. it also reveal that in 2007, water body covered 23.38%, Vegetation covers 31.33%, cultivated land covered 33.21%, built up land also increase to 11.22%, weed covered 0.67% and bare land covered 0.19% and in 2017 water body has increase to 24.38%, vegetation had reduce to29.53%, cultivated land has also increase to 40.95%, built up also increase to 12.65%, weeds also increase to 0.26%.



***Landuse 1997***

***Landuse 2007***

***Landuse 2017***

# Figure 4.1: Kainji Landuse Classification of 1997, 2007 and 2017

Table 4.1 shows three classified images of 1997, 2007 and 2017, respectively, it reveals that some parts of the area have not been subjected to changes (static) between 1997 and 2017. Table 4.2 shows the trend in terms of the area coverage and the percentage of each class of the area from 1997 to 2017. This means that some parts of the areas surrounding Kainji dam has been subjected to changes. This was also revealed in Figure 4.1 in 2007, settlement and human activities in around the dam were very little, Extensive agriculture/grazing land and intensive agriculture had the highest percentage changes of




41.78 and 35.45%, respectively, between 1997 and 2017, though, while extensive agriculture changes positively, intensive agriculture recorded negative changes. From 1997 through 2007 to 2017, extensive agriculture/grazing land reduced drastically which is a result of the policy of the Federal Government against grazing in the area.

# Table 4.1: Summary of Kainji Landuse Classification 1997-2017

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Land cover** | **1997**  **Area (Hectares)** | **Area (%)** | **2007**  **Area (Hectares)** | **Area (%)** | **2017**  **Area (Hectares)** | **Area (%)** |
| Water Body | 9.5 | 22.12 | 10. 10. | 23.38 | 10.13 | 24.38 |
| Vegetation | 192.5 | 44.15 | 136.6 | 31.33 | 136.5 | 24.53 |
| Cultivated Land | 133.1 | 23.42 | 154.9 | 33.21 | 147.5 | 38.95 |
| Built-up | 99.9 | 9.62 | 140.7 | 11.22 | 135.5 | 12.06 |
| Weeds | 4.5 | 0.56 | 7.2 | 0.67 | 9.1 | 0.71 |
| Bare land | 1.6 | 0.13 | 2.1 | 0.19 | 2.3 | 0.26 |

Figure 4.2 shows the spatial temporal analysis of Shiroro dam and identify the changes in the area extent of the different land-use type involved evaluation of remotely sensed satellite imagery for the period of 1997, 2007 and 2017. It shows that Shiroro area covers a landmass of 72km2. The built-up area in 1997 was low while vegetal cover was high because it has not been tempered with much. It also reveals that built-up area covered 9.7km2 (13.4%), vegetated land covered 7.9km2 (11%), cultivated covered 35.3km2 (49%), bareland land covered 8.6km2 (12%) and water body covered 10.5km2 (14.6%) in

1997. The analysis that in 2007, Built-up area had increased from 9.7km2 (13.4%) in 1995 to 28.5km2 (39.6%) in 2007, vegetated land increased from 7.9km2 (11%) in 1997 to 8.6km2 (12%) in 2007, cultivated surface decreased from 35.3km2 (49%) in 1997 to 23km2 (32%) in 2007, bareland land decreased from 8.6km2 (12%) in 1997 to 4.5km2 (6.2%) in 2007 and water body decreased from 10.5km2 (14.6%) in 1997 to 7.3km2 (10.2%) in 2007.



***Landuse 1997***

***Landuse 2007***

***Landuse 2017***

Figure 4.2: Shiroro Landuse Classification of 1997, 2007 and 2017




# Table 4.2 Summary of Shiroro Landuse Classification 1997-2017

|  |  |  |  |
| --- | --- | --- | --- |
| land cover | 1996 | 2007 | 2017 |
| Built-up area | 9.7 | 28.5 | 38.9 |
| Bare land | 7.9 | 8.6 | 5.5 |
| Vegetated land | 35.3 | 23.0 | 10.6 |
| Cultivated land | 8.6 | 4.5 | 11.7 |
| Water body | 10.5 | 7.3 | 5.3 |
| Weeds | 3.7 | 4.1 | 4.5 |

From Table 4.2, built-up area changed from 9.7km2 (13.4%) in 1997 to 28.5km2 (39.6%) in 2007 and increased to 38.9km2 (54%) in 2017; vegetated land changed from 7.9km2 (11%) in 1997 to 8.6km2 (12%) in 2007 and decreased to 5.5km2 (7.7%) in 2017; vegetated changed from 35.3km2 (49%) in 1997 to 23.0km2 (32%) in 2007 and further decreased to 10.6km2 (14.7%) in 2017; farm land changed from 8.6km2 in 1995 to 4.5km2 (6.2%) in 2007 and increased to 11.7km2 (16.3%) in 2017 and water body reduced from 10.5km2 (14.6%) to 7.3km2 (10.2%) and further decreased to 5.3km2 (7.3%) in 2017.

# Comparative analysis of the Spatial-temporal characteristics of the dams

It is important to compare the extent of spatial temporal changes of Kainji and Shiroro dam so as to assess the areas in any desired unit and percentages for proper land-use planning. The image calculator of the Idrisi software was used to determine the extent of spatial temporal changes around Kainji and Shiroro dam. The image shows a typical growing season pattern covering the time-series representative the study area (Figure 4.3 and Figure 4.4).






NDVI 1997

NDVI 2007

NDVI 2017

Figure 4.3 Kainji NDVI analysis between 1997, 2007 and 2017

The NDVI shows variations on spatial temporal characteristics such as natural vegetation and agricultural land, the index ranges between 0.81 high and -0.54 low, it indicated that the southern part clearly shows a more intensive agricultural activity while the southern part show a low vegetation biomass based on the NDVI. It was revealed that in 2007 the spatial temporal characteristics has reduced compared to 1997 and this also has a negative effect on other landuse classes. In 2017 the spatial temporal characteristics as the coefficient of variation (COV) of the study area where more variation exists along the Dam.



NDVI 1997

NDVI 2007

NDVI 2017

Figure 4.4 Shiroro NDVI analysis between 1997, 2007 and 2017


Figure 4.4 shows a serious negative effect on the spatial temporal characteristics of Shiroro in 2017, a total area of 205.2558 km2 representing 4.75% of the area has been

captured by the reservoir between 1997 and 2017. This means that the area is actually expanding as has earlier been reported by Abiodun (2009) and Ikusemoran (2009a). The spatial temporal characteristics has also lost a total area of 943.2975 km2 (21.83%) between 1997 and 2017. Cultivated land is the degrading factor of the area as 1587.7759 km2 (36.75%) of the area have been lost to intensive agriculture between 1997 and 2017.

# Spatial variations of rainfall, reservoir inflow, reservoir elevation, evaporation and turbine discharge in Kainji

# Trend analysis of rainfall

The intra seasonal variation of rainfall over Kainji shows that rainfall generally begins in March / April, increase until the mount of November and decrease thereafter until cessation takes place completely in November. Figure 4.5 shows that about 50% of the annual rainfall total accumulates in three heaviest rainy months of July, August and September and lowest in the months of January, February and December. There is thus a marked dry and rainy seasons.



10000

9000

8000

7000

6000

5000

4000

3000

2000

1000

0

JAN FEB MAR APR MAY JUN JUL AUG SEP OCT NOV DEC

**Month**

**Mean Rainfall**

Figure 4.5: Mean Monthly Rainfall of Kainji

Figure 4.6 shows rainfall trend of Kainji between 1987 – 2017 was also analyzed; the deviation of mean annual values of rainfall over thirty (30) years was shown in Figure

4.6. The deviation of rainfall negative between 1987and 1988. Between 1989 and 1991, the deviations is positive over a period of five years. On decadal basis, the years 1991 and 1994 have the highest deviations while the remaining years have very low deviations. The rainfall deviations increased between 1998 and 1999. On decadal basis, the years 1998, 1999, 2004, and 2006 have positive rainfall deviations while the remaining years have negative and least rainfall deviations. Between the year 2008 and 2016, the rainfall deviations were positive in the year 2008, 2010 and 2011. However, the deviations were lowest in the year 2012 and 2014. The years 2009, 2013, 2015 and 2016 have a negative rainfall deviation within the area. This implies the rainfall between 1987 and 2017 have a slightly decreasing trend (graphically) in the study area. The result of the study conclude that as water is a main component for generating electricity in Kainji the slight decreasing trend in rainfall will have significant effect on energy generation.

2

1.5

1

0.5

0

**Rainfall deviation (mm)**

-0.5

-1

-1.5

-2

-2.5

**Year**



# Figure 4.6 Rainfall deviation

62



Table 4.3 shows the trend of rainfall over thirty year. The months of January, February, March, April, May, July, August, September , November, December have Z values less than 1.96 meaning that these months have insignificant trend. The months of June and October have z values greater than 1.96. This implies that the trends were significant. The month of October has a positive trend while the month of June has a negative trend. On annual basis, the rainfall records have decreasing trend.

# Table 4.3 Trend analysis of rainfall between 1987 and 2017 using Mann Kendall test

|  |  |  |  |
| --- | --- | --- | --- |
| Month | tau | S value | Zvalue |
| Jan | 0.0713 | 31 | 0.6612 |
| Feb | 0.0506 | 22 | 0.4629 |
| March | -0.0989 | -43 | -0.9257 |
| Apr | 0.0667 | 29 | 0.6172 |
| May | -0.0483 | -21 | -0.4408 |
| June | -0.2552 | -111 | -2.4246 |
| July | -0.0345 | -15 | -0.3086 |
| August | -0.2046 | -89 | -1.9397 |
| Sept | 0.2046 | 89 | 1.9397 |
| Oct | 0.3195 | 139 | 3.0417 |
| Nov | 0.1563 | 68 | 1.4768 |
| Dec | 0.0667 | 29 | 0.6172 |

# Trend analysis of Evaporation

Evaporation from the land surface includes evaporation from open water, soil, shallow groundwater, and water stored on vegetation, along with transpiration through plants. Figure 4.7 shows the mean monthly evaporation for Kainji, it was discovered that evaporation was high in the first three months (January, February and March), and started decreasing from April to July. It pick up again in August and September and slighting down in September and rise again in November and December. It was discovered that July has the lowest mean evaporation (3.24) while December has the highest (15).



16

15

13.75

14

12.97

11.74

12.03

12

10.72

10

8.39

7.55

8

6.47

6

5.33 5.4

4

3.24

2

0

**Month**

**Evaporation**

# Figure 4.7: Mean Monthly Evaporation in Kainji Dam

The rate of evaporation from the land surface is driven essentially by meteorological controls, mediated by the characteristics of vegetation and soils, and constrained by the amount of water

available. Climate change has the potential to affect all of these factors in a combined way that is not yet clearly understood with different components of evaporation affected differently.

Annual trend of evaporation was presented in Figure 4.8, it revealed the deviation for mean annual values of evaporation over thirty (30) year in the study area. There were stable deviations between 1987 and 1991. The evaporation deviation was increased in the years 1995 but it reduced drastically between 1993 and 1994. In the year 1995, the deviation was very high. On the decadal basis, the years 1996 and 1997 have negative and least temperature deviation. On decadal basis, the year 1998 and 2000 have the highest temperature deviations while the years 1999 and 2001 have the least deviations. Between 2012 and 2008, the study showed that the deviations have lowest values with a negative pattern. Furthermore, the year 2010 has a positive and least value while the remaining years showed negative deviations.

2.5

2

1.5

1

0.5

**Evaporation deviation (mm)**

0

198719881989199019911992199319941995199619971998199920002001200220032004200520062007200820092010201120122013201420152016

-0.5

-1

-1.5

-2

**Year**

# Figure 4.8 Evaporation deviation

66

Table 4.4 showed the trend analysis of evaporation over years. The months of April, May, June, July, September, October, January, February and March between 1987 and 2017 have Z values𝑔𝑟𝑒𝑎𝑡𝑒𝑟 𝑡ℎ𝑎𝑛 1.96. This study showed that these months have significant trend. This means that the month of September has a positive trend while the remaining months have negative trends. The month of August, November and December have 𝑍 𝑣𝑎𝑙𝑢𝑒𝑠 𝑙𝑒𝑠𝑠 𝑡ℎ𝑎𝑛 1.96 meaning that there were no trends for these months.


# Table 4.4 Trend analysis of evaporation between 1987 and 2017

|  |  |  |  |
| --- | --- | --- | --- |
| Month | tau | S value | Z value |
| Jan | -3540 | -154 | -3.3724 |
| Feb | -0.4368 | -190 | -4.1659 |
| Mar | -0.4759 | -207 | -4.5406 |
| Apr | -0.5425 | -236 | -5.1798 |
| May | -0.5149 | -224 | -4.9153 |
| June | -0.2506 | -109 | -2.3805 |
| July | -0.4138 | -180 | -3.9454 |
| Aug | 0.154 | 67 | 1.4547 |
| Sep | 0.3379 | 147 | 3.2181 |
| Oct | -0.446 | -194 | -4.254 |
| Nov | -0.0874 | -38 | -0.8155 |
| Dec | -0.1195 | -52 | -1.1241 |

# Trend analysis on reservoir inflow

Outlet usually is expressed as stream flow; over durations of a month or more, it usually is expressed as runoff. Runoff tends to increase where precipitation has increased and decrease where it has fallen over the past few years. Figure 4.9 shows the reservoir inflow of Kainji Dam. It reveals that January has a mean inflow of 1145 and it was decrease to 580 in February. The decrease

continue until June with mean inflow of 79, it raise in July to 390 and continue raising to 1335 in December. Flows have increased in recent years in Kainji dam, Variations in flow from year to year have been found to be much more strongly related to precipitation changes than to temperature changes. A major and unprecedented shift in streamflow from spring to winter has been associated not only with a change in precipitation totals but more particularly with a rise in temperature: Precipitation has fallen as rain, and therefore has reached rivers more rapidly than before.



1376 1376

1400

1323 1335

1200

1145

1061

1000

800

580

600

390

400

241

200

83

50

79

0

JAN FEB MAR APR MAY JUN JUL AUG SEP OCT NOV DEC

**Month**

**Mean Inflow**

# Figure 4.9: Mean Monthly Reserviour inflow in Kainji

Figure 4.10 revealed that the deviation for mean monthly reservoir inflow over thirty (30) year. Between 1987 and 1993, the reservoir inflow deviations decreased with negative values. In addition, the years 1994, 1995 and 1996 have positive deviations. Furthermore, the deviation reduced in the year 1997. Between 1998 and 2008, the reservoir inflow deviations were high in the year 1998, 1999 but reduced in the year 2000 with a little increase in the year 2001 but drastically reduced in the year 2002. The deviations increased in the year 2003 but reduced in 2004

with a negative deviation values in the year 2005 and 2006. The deviation increased from 2007 to 2008 but reduced in 2009 and later increased in the year 2010. The year 2011 and 2016 have a positive deviation while the years 2012, 2013, 2014 and 2015 have negative deviations. Graphically, the study showed that the reservoir inflow has an positive trend. The study revealed that even though the direction of the rainfall was reduced between 1987 and 2017 but the generated runoff around the catchment area still increases the trend of reservoir inflow.

**Reservior inflow deviation (Mm3)**

# Figure 4.10 Reservoir inflow deviation



2

1.5

1

0.5

0

-0.5

-1

-1.5

-2

**year**

70

Table 4.5 shows the trend analysis of reservoir inflow over thirty years. The monthly reservoir inflow records between April and July have 𝑍 𝑣𝑎𝑙𝑢𝑒𝑠 𝑙𝑒𝑠𝑠 𝑡ℎ𝑎𝑛 1.96 had no trend. This implies that the trends were insignificant. Furthermore, the months of August and March have Z values greater than 1.96 which shows that these months have significant trend. Properly the months that reservoir inflow is significant is due to increase in rainfall and runoff from other rivers outside Kainji, while months that reservoir inflow is insignificant may be due to very high rainfall that leads to erosion because of indiscriminate farming from the upstream which prevent runoff, these will lead to sedimentation deposit in the reservoir and these will reduce the life span of the reservoir and also have effect on energy generation.

# Table 4.5 Trend analysis of reservoir inflow between 1987 and 2017

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Month | tau | S value |  | Z value |
| Jan |  | 0.3356 | 146 | 3.196 |
| Feb |  | 0.3793 | 165 | 3.6148 |
| Mar |  | -0.3195 | 139 | 3.0417 |
| Apr |  | 0.1471 | 64 | 1.3886 |
| May |  | 0.1908 | 83 | 1.8074 |
| June |  | 0.1149 | 50 | 1.08 |
| July |  | 0.1655 | 72 | 1.565 |
| Aug |  | 0.3793 | 165 | 3.6148 |
| Sep |  | 0.3379 | 147 | 3.2181 |
| Oct |  | 0.4759 | 207 | 4.5406 |
| Nov |  | 0.3448 | 150 | 3.2842 |
| Dec |  | 0.3402 | 148 | 3.2401 |

* 1. **Spatial variations of rainfall, reservoir inflow, reservoir elevation, evaporation and turbine discharge in Shiroro**

# Spatial variation of rainfall in Shiroro

Rainfall is the main driver of variability in the water balance over space and time, and changes in precipitation have very important implications for hydrology and water resources. Hydrological variability over time in a catchment is influenced by variations in precipitation over daily, seasonal, annual, and decadal time scales. Figure 4.11: Monthly rainfall distribution in Shiroro Dam

350

300

250

200

150

100

50

0

Jan Feb Mar Apr May Jun Jul Aug Sep Oct Nov Dec

**Figure 4.11: Monthly Rainfall Distribution at Shiroro Dam**

The intra seasonal variation of rainfall over the catchments is shows that rainfall generally begins in March / April, increase until the mount of September and decrease thereafter until cessation takes place completely in November. About 50% of the annual rainfall total accumulates in two heaviest rainy months of July and August and lowest in the months of January, February and December. There is thus a marked dry and rainy seasons. The former generally lasts for about five

to six months, while the latter lasts for about six to seven months. The sensitivity of the river Kaduna flow to rainfall does not usually start until July when traditionally, the months of September / early October marks the peak of the inflow. The peak inflow immediately following accumulated peak rainfall period may be attributed to the time-lag factor between rainfall and peak flow.

On a yearly basis, noticeable oscillations were recorded. Rainfall picked up in 1992. It went down in 1993 and picked up again for two consecutive years (1994 and 1995). The year 1996 witnessed a downturn in the amount of rainfall received. From 1997 to 2001 also marked another period of increase in rainfall amount. The years 2002 to 2005 showed rainfall oscillating downwards.It should be noted that the yearly distribution of rainfall over the Shiroro reservoir hovers between 1000mm and 1450mm with a mean of 1200mm. The implication of this rainfall scenarios is that no meaningful variation in recorded at this location during the study period. Figure 4.12: Annual Rainfall Distribution

1600

1400

1200

1000

800

Rainfall

600

400

200

Figure 4.2 Illustrates the Annual Distribution of Rainfall over the Shiroro Dam

0

1987 1988 1989 1990 1991 1992 1993 1994 1995 1996 1997 1998 1999 2000 2001 2002 2003 2004 2005 2006 2007 2008 2009 2010 2011 2012 2013 2014 2015 2016 2017

Year

Figure 4.12: Annual Rainfall Distribution

74

# 4.4.2 Trend analysis of evaporation in Shiroro

Evaporation from the land surface includes evaporation from open water, soil, shallow groundwater, and water stored on vegetation, along with transpiration through plants. The rate of evaporation from the land surface is driven essentially by meteorological controls, mediated by the characteristics of vegetation and soils, and constrained by the amount of water available. Climate change has the potential to affect all of these factorsin a combined way that is not yet clearly understoodwith different components of evaporation affected differently.

160

140

120

100

80

60

40

20

0

Jan Feb Mar Apr May Jun Jul Aug Sep Oct Nov Dec

Months

Evaporation

# Figure 4.13 Illustrates of monthly evaporation in Shiroro dam

The primary meteorological controls on evaporation from a well-watered surface are the amount of energy available the moisture content of the air and the rate of movement of air across the surface. Increasing temperature generally results in an increase in potential evaporation, largely because the water-holding capacity of air is increased. Changes in other meteorological controls

may exaggerate or offset the rise in temperature, and it is possible that increased water vapor content and lower net radiation could lead to lower evaporative demands.

The effects of climate change have concentrated on potential changes on streamflow and runoff. The distinction between “streamflow” and “runoff” can be vague, but in general terms Stream flow is water within a river channel, usually expressed as a rate of flow past a point typically in m3 s-1 whereas runoff is the amount of precipitation that does not evaporate, usually expressed as an equivalent depth of water across the area of the catchment. A simple link between the two is that runoff can be regarded as stream flow divided by catchment area at Shiroro Dam.

# Table 4.6: Mean Monthly Rainfall and Evaporation at Shiroro dam

**Annual**

**(mm)**

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Jan** | **Feb** | **Mar** | **Apr** | **May** | **Jun** | **Jul** | **Aug** | **Sep** | **Oct** | **Nov** | **Dec** | **Total** |
| **Rainfall (mm)** 0 | 1 | 18 | 65 | 142 | 221 | 173 | 305 | 254 | 78 | 0 | 0 | **1253** |
| **Evaporation**  142 | 138 | 121 | 117 | 98 | 66 | 52 | 48 | 50 | 61 | 84 | 135 | **1112** |
| **Variation in**  -142 | -137 | -103 | -52 | 44 | 155 | 121 | 257 | 204 | 17 | -84 | -135 | **141** |

**Values**

Figure 4.14: Relationship between Rainfall and Evaporation of Shiroro Dam

350

300

250

200

150

100

50

0

Jan Feb Mar Apr May Jun Jul Aug Sep Oct Nov Dec

**Months**

Rainfall (mm)

**Rainfall/Evaporation (mm)**

Figure 4.14 illustrate seasonal moisture distribution at Shiroro dam. Figure 4.14 indicates periods of moisture deficit which is between November and March and another period of moisture surplus which is between April and October when the rainfall is in excess of the evaporation. However, at any point in time, water is available in the reservoir.



600

500

400

300

200

100

0

JAN FEB MAR APR MAY JUN JUL AUG SEP OCT NOV DEC

**Months**

**Inflow m3/s**

Figure 4.15 Average Monthly Inflow

**Outflow (m3/s**

# Figure 4.16 Monthly Average Outflow



450

400

350

300

250

200

150

100

50

0

JAN

FEB MAR APR MAY JU**M**N**onth**JU**s**L

AUG SEP OCT NOV DEC

Outlet usually is expressed as streamflow; over durations of a month or more, it usually is expressed as runoff. In some countries, “runoff” implies surface runoff only and does not include the contribution of discharge from groundwater to flow, but this is a narrow definition of the term.

Runoff tends to increase where precipitation has increased and decrease where it has fallen over the past few years. Flows have increased in recent years in Shiroro dam, Variations in flow from year to year have been found to be much more strongly related to precipitation changes than to temperature changes. A major and unprecedented shift in streamflow from spring to winter has been associated not only with a change in precipitation totals but more particularly with a rise in temperature: Precipitation has fallen as rain, and therefore has reached rivers more rapidly than before.

500

450

400

350

300

Inflow / Outflow

250

200

150

100

50

0

1987 1988 1989 1990 1991 1992 1993 1994 1995 1996 1997 1998 1999 2000 2001 2002 2003 2004 2005 2006 2007 2008 2009 2010 2011 2012 2013 2014 2015 2016 2017

Year

Inflow out Flow

Figure 4.17 Annual Distribution of Inflow and Outflow into and from Shiroro Dam

79

However, it is very difficult to identify trends in hydrological data, for several reasons. Records tend to be short, and many data sets come from catchments with a long history of human intervention. Variability over time in hydrological behavior is very high, particularly in drier environments, and detection of any signal is difficult. Variability arising from low- frequency climatic rhythms is increasingly recognized, and researchers looking for trends need to correct for these patterns.



350

300

250

200

y = 14.026x

R² = -0.028

150

100

50

0

0

2

4

6

8

10

12

14

**Months**

**Rainfall (mm)**

Figure 4.18: Monthly Rainfall Correlation



1200

y = 45.191x

R² = 0.1692

1000

800

600

400

200

0

0

2

4

6

8

10

12

14

**Months**

**Inflow m3/s**

Figure 4.19: Monthly inflow

Figure 4.20: Monthly outflow



600

500

y = 40.892x

R² = -9.805

400

300

200

100

0

0

2

4

6

8

10

12

14

**Months**

**Outflow (m3/s)**

The effects of climate change on the magnitude of annual runoff and flows through the year are much less consistent than the effect on Dam flow timing because they depend not on the temperature increase but on the change in precipitation. In general, precipitation increases in high-latitude areas under most scenarios, but in lower latitudes precipitation may decrease. Hydrological regimes in these regions are dominated by the seasonal cycles of rainfall and evaporation; inflow and outflow are not important. Here, climate change tends to affect the magnitude of flows in different seasons by an amount that depends on the change in rainfall and may lead to an exaggerated seasonal cycle, but it generally does not affect the timing of flows through the year. Low flows tend to occur during raining, and changes in low-flow frequency are closely related to changes in the balance between rainfall and evaporation. Temperate, rainfall would decline with global warming, leading to a reduction in low flows.

The detailed effect of a given change in climate, however, depends to a large extent on the geological characteristics of Shiroro have indicated that in catchments with considerable

groundwater, changes in dry flows are largely a function of the change not in rainfall but in rainfall during the winter recharge season. Dam are particularly vulnerable to changes in climate parameters. Variations in air rainfall and other meteorological components directly cause changes in evaporation, water balance, Dam level, hydrochemical and hydrobiological regimes, and the entire lake ecosystem. Under some climatic conditions, lakes may disappear entirely.

# CHAPTER FIVE

* 1. **CONCLUSION AND RECONMENDATIONS**

# Conclusion

The comparative analysis of spatial temporal variations in hydrological parameters at Kainji and Shiroro Dams in Niger State, Nigeria was conducted using data on rainfall, evaporation, reservoir inflow and outflow for the period of thirty years from Kainji and Shiroro Hydropower Station. The community which is the host of the dam water has been revealed to be expanding- causing fear of dam collapse, the natural vegetation is rapidly decreasing- putting, water hyacinth has recently captured some parts of the dam and despite numerous efforts by the government and research institute, the weeds as at 2017, still covered more than 40 km2 of the dam surface, intensive agriculture that was very minimal in 1985 was discovered to have captured more than 40% of the dam basin. The data collected was used to show the trend of each parameter for the time frame of study. Firstly summary statistics of all variables was conducted to know if the mean, annual mean, maximum minimum and overall total amount of each variable was computed to check if the data collected are evenly distributed. Mann Kendall’s was used on all variables to show the trends and deviations for each variable using Excel package. The comparatively analyses rainfall, evaporation, and reservoir inflow in each of the dam. The findings of these research show that reservoir inflow experienced tremendous fluctuations over the years of study.

The rainfall, evaporation and reservoir inflow within Kainji and Shiroro dam were subjected to Mann Kendall, Design expert analyses. The trends of the variables for the time frame of study were shown using trend line. The analyses revealed that evaporation show a negative trend, and a slight decrease in rainfall. while reservoir inflow pattern shows a increasing

trend, due to order river channel flowing from outside the dams but if there is a slight decrease it might not be noticeable

# Recommendations

In relations to the findings of this study, the following recommendations became essential.

* + 1. The Government should embark on Enhancement in the measurement, monitoring, forecasting, and knowledge of the hydrologic system.
    2. It is recommended that dam operators optimize the release of water from Kainji and Shiroro dam and ensure continuous monitoring of changes in hydro meteorological variables to provide early warning systems for effective performance of the dam and to protect downstream environment.
    3. The government should strengthen laws, policies and measures relevant to addressing climate variability, as this will help in limiting global warming, which is the reason behind drought and low precipitation.
    4. Reduction of the current variability by means of increased storage capacity by constructing buffer dams and reservoirs in order to store excess runoff during the periods of high flows.
    5. The government should carry out wide-ranging review of existing national water resources master plan. The new plan should seriously consider recent phased development and management of particular problems. While a financial plan should be adopted in setting out annual budgetary allocations to relevant water development and energy projects.

# REFERENCES

Abaje, I. B., Achiebo, P. J., & Matazu, M. B. (2018). Spatial-temporal analysis of rainfall distribution in Kaduna State, Nigeria. *Ghana Journal of Geography*, *10*(1), 1-21.

Adegbehin, A. B., Yusuf, Y. O., Iguisi, E. O., & Zubairu O. D. (2016). Reservoir inflow pattern and its effects on hydroelectric power generation at the Kainji Dam, Niger State, Nigeria. *WIT Transactions on Ecology and the Environment*, 203, 233-244. Retrieved from https://[www.ars.usda.gov/people-locations/person?person-id=335](http://www.ars.usda.gov/people-locations/person?person-id=335)

Akinsanola, A. A., & Ogunjobi, K. O. (2014). Analysis of rainfall and temperature variability over Nigeria. *Global Journal of Human-Social Science Research* 18 (5) 167-184

Apalando, M. A. (2012). Impact of climate change on streamflow of the Kainji lake basin using statistical and artificial neural network (ANN) Methods. Master thesis submitted to the University of Ilorin.

Bibi, U. M., Kaduk, J., & Balzter, H. (2014). Spatial-temporal variation and prediction of rainfall in northeastern Nigeria. *Climate*, *2*(3), 206-222.

Bower, M. L. (2004). *Assessment of the Potential Effects Water and Adaptations for Climate Change in Europe*: The Europe ACACIA Project. Jackson Environment Institute, University of East Anglia, Norwich, UK, 320 pages.

Camberlin, P., Brovin, V., Claussen, M.and Ganopolski, A. (2001). “On the Stability of the Atmosphere Vegetation System in the Sahara/Sahel, Region”. *Journal of Geophysical Research*. 103 (D24) 31613- 31624.

Cigizoglu, H. K., Bayazit, M., & Onoz, B. (2005). Trends in the maximum, mean, and low flows of Turkish rivers. *Journal of Hydrometeorology*, 6(3), 280-290, doi: <http://dx.doi.org/10.1175/JHM412.1>

Collins, P., Tim, Paul, and Bamzai, A.S. (2010). Relationship between Snow Cover Variability and Arctic Oscillation index on a hierachy of time scales. *International Journal of Climatology.* 23: 131-142.

Corzo Perez ,G. A., M. H. J. van Huijgevoort, F. Voß, and H. A. J. van Lanen, (2011) “On the spatio-temporal analysis of hydrological droughts from global hydrological models,” *Hydrology and Earth System Sciences*, 15, ( 9) 2963–2978.

Cristiano, E., Veldhuis, M. C. T., & Giesen, N. V. D. (2017). Spatial and temporal variability of rainfall and their effects on the hydrological response in urban areas–a review. *Hydrology and Earth System Sciences*, 21(7), 3859-3878.

Egor, A. O., Osang, J. E., Uquetan, U. I., Emeruwa, C., & Agbor, M. E. (2015). *Inter-Annual Variability of Rainfall in Some States of Southern Nigeria. Journal of Environmental Sciences 8 (6) 111-129*

Ehigiator, M. O., Oladosu, O. S., & Ehigiator–Irughe, I. R. (2017). Determination of volume and direction of flow of Kainji Reservoir using hydro-geomatics techniques. *Nigerian Journal of Technology*, 36(4), 1010-1015. Retrieved from <http://www.nijotech.com/index.php/nijotech/article/view/1466/0>

Ezemonye, M. N. ***&*** *Emeribe, C. N.* (2015). Spatial and temporal patterns of climatic change in the Sokoto-Rima River Basin, Sudano-Sahel region, Nigeria. *European Scientific Journal*, *11*(26) 216-222

Goswami, B. N., Venugopal, V., Sengupta, D., Madhusoodanan, M., Xavie, P.K. (2006). *Increasing trend of extreme rain events over India in a warming environment. Science,* 314 (5804), 1442–1445.

Goswami, P., & Himesh, S. (2002). Coupled atmospheric–hydrologic models to forecast spatio-temporal variability of water resources. Retrieved from <http://www.csir4pi.in/cmmacs/Publications/tech_rep/trcm0201r.pdf>

Guntner, A., J. Stuck, S. Werth, P. Do¨ll, K. Verzano, and B. Merz (2007). A global analysis of temporal and spatial variations in continental water storage, *Water Resource* 43, W05416, doi:10.1029/2006WR005247.

Harrison G. P., Whittington H. W. and Gundry S. W. (2014). Climate change impacts on hydroelectric power, UK, 2(1), 1-5

Ifabiyi, I. P., & Ashaolu, E. D. (2015). Spatio-temporal pattern of rainfall distribution over Ilorin metropolis, Nigeria. *Scientia Africana*, *14*(2), 229-247.

Ifeanyi, C. (2011). Implications of Climate Variability on Water Resources of Nigeria: a review. *Journal of Geography and Regional Planning*, *4*(13), 678-682.

IPCC. *Climate Change (2001) The Physical Science Basis. Contribution of Working Group I to the Fourth Assessment Report of the Intergovernmental Panel on Climate Change*; IPCC: Geneva, Belgium.

Javari, M. (2016). Spatial-temporal Variability of Seasonal Precipitation in Iran. The Open Atmospheric Science Journal, 10, 84-102. DOI: 10.2174/1874282301610010084

John, C.J. & James, T.T. (2011) *Annual Energy Outlook*. United States energy information administration. Available from [www.eia.gov/forecasts/aeo](http://www.eia.gov/forecasts/aeo).

Krasovskaia, H. E. and Gottsschalk, S. P. (2002). “Land-Ocean - Atmosphere Interactions and Monsoon Climate Change: A Paleo-perspective”, in Schulze, E. D., Harrison, S. P., Heimann, M. *In the Climate System.* San Diego, Academic Press, pp. 73-86.

Kuchment, L. S. (2004). The hydrological cycle and human impact on it. *Water resources management*. Retrieved from <http://www.eolss.net/ebooks/Sample%20Chapters/C07/E2-16-10-01.pdf>

Kuti, I. A., Animashaun, I. M., Olawale, B., & Abdullahi, S. (2015). Trend analysis of hydro- meteorological data for river Kaduna at Shiroro dam site, Niger State Nigeria*. Journal of Scientific Research & Reports*, *8(5): 1-12,*

Lee, S. & Kim, S. U. (2017). Quantification of hydrological responses due to climate change and human activities over various time scales in South Korea. *Water,* 9(34), 1-22; DOI: 10.3390/w9010034.

Lloyd-Hughes, B. L. C. Shaffrey, P. L. Vidale, and N. W. Arnell, “An evaluation of the spatiotemporal structure of large-scale European drought within the HiGEM climate model,” *International Journal of Climatology,* vol. 33, no. 8, pp. 2024–2035, 2013. View at Publisher · View at Google Scholar · View at Scopus

Luo, Y., Wang, Z., Liu, X., and Zhang, M. (2014). Spatial and temporal variability of precipitation in haihe river basin, China: *characterization and management implications. advances in meteorology*, 1(1), 1-9.

<http://dx.doi.org/10.1155/2014/143246>

Nan, Y., Bao-hui Men, & Chun-kun, L. (2011). Impact analysis of climate change on water resources. *Procedia Engineering*, 24, 643–648. doi:10.1016/j.proeng.2011.11.2710. Retrieved from https:/[/www.scienc](http://www.sciencedirect.com/science/article/pii/S1877705811055)e[direct.com/science/article/pii/S1877705811055](http://www.sciencedirect.com/science/article/pii/S1877705811055) 627

Odjugo, P. (2010). The impact of climate change on water resources: global and Nigerian analysis. *FUTY Journal of the Environment*, 4(1). doi:10.4314/fje.v4i1.48005. Retrieved from <http://www.gracelinks.org/2380/the-impact-of-climate-change-on-> water-resources

Oguntunde, P. G., Abiodun, B. J., & Lischeid, G. (2012). Spatial and temporal temperature trends in Nigeria, 1901–2000. *Meteorology and Atmospheric Physics*, *118*(1-2), 95- 105.

Ojha, R., Pathak, S., Bhunya, P. K., Jain, S. K., & Adeloye, A. J. (2017). Climate change pattern and its effect on hydrologic cycle: A Review. *Sustainable Water Resources Management*, 293–316

Oki, T. (2006). The hydrologic cycles and global circulation. *Encyclopedia of hydrological sciences* 6 (11) 76-93

Ovie, S. I., & Adeniji, H. A. (1994). Zooplankton and environmental characteristics of Shiroro Lake at the extremes of its hydrological cycle. *Hydrobiologia,* 286(3), 175- 182.

Peleg, N., Blumensaat, F., Molnar, P., Fatichi, S., and Burlando, P. (2017). Partitioning the impacts of spatial and climatological rainfall variability in urban drainage modelling. *Hydrology Earth System Science*, 21, 1559–1572, [https://doi.org/10.5194/hess-21-](https://doi.org/10.5194/hess-21-1559-2017) [1559-2017](https://doi.org/10.5194/hess-21-1559-2017),

Sakka, M. (2011). Application and comparison of two analytical tools of decision support for the management of resources in a river basin in Tunisia. Ph.D. submitted to Tuscia University of Viterbo

Saraiva Okello, A. M. L., Masih, I., Uhlenbrook, S., Jewitt, G. P. W., Van der Zaag, P., & Riddell, E. (2015). Drivers of the spatial and temporal variability of streamflow in the Incomati River basin. *Hydrology and Earth System Sciences*, 19(2), 657-673.

Shen, C and Qiang, H. (20014). Spatial and temporal variation of annual precipitation in a River of the Loess Plateau in China. *Journal of Applied Mathematics*, 1-11. Retrieved from https://[www.hindawi.com/journals/jam/2014/827120/](http://www.hindawi.com/journals/jam/2014/827120/)

Shen, C., & Qiang, H. (2014). Spatial and temporal variation of annual precipitation in a river of the loess plateau in China. *Journal of Applied Mathematics*, 1(1), 1-11. <http://dx.doi.org/10.1155/2014/827120>

Shiklomanov, A. I., R. B. Lammers, M. A. Rawlins, L. C. Smith, and T. M. Pavelsky (2007). Temporal and spatial variations in maximum river discharge from a new Russian data set, *Journal of Geophysics Research*., 112, G04S53, doi: 10.1029/2006JG000352.

Sohoulande Djebou, D. C. and Singh, V. P. (2016). Impact of climate change on the hydrologic cycle and implications for society. *Environment and Social Psychology*, 1 (1): 36–49. <http://dx.doi.org/10.18063/ESP.2016.01.002>.

Sohoulande Djebou, D. C., Singh, V. P. and Frauenfeld, O. W. (2015). Vegetation response to precipitation across the aridity gradient of the southwestern United States. *Journal of Arid Environments*, 115: 35–43. <http://dx.doi.org/10.1016/j.jaridenv.2015.01.005>

Stagl, J., Mayr, E., Koch, H., Hattermann, F. F., & Huang, S. (2014). Effects of climate change on the hydrological cycle in central and eastern Europe. In *Managing Protected Areas in Central and Eastern Europe Under Climate Change* (pp. 31-43). Springer, Dordrecht.

Stahl, K., H. Hisdal, J. Hannaford (2010)., “Streamflow trends in Europe: evidence from a dataset of near-natural catchments,” *Hydrology and Earth System Sciences*, 14 (12), 2367–2382.

Usman, A. & Ifabiyi, I. P. (2012). Socio-economic analysis of the operational impacts of Shiroro hydropower generation in the lowland areas of middle river niger. *International Journal of Academic Research in Business and Social Sciences*, 2(4),

57. Retrieved from <http://www.hrmars.com/admin/pics/685.pdf>

Warwade P., Tiwari S., Ranjan S., Chandniha S.K., Adamowski J. (2018). Spatio-temporal variation of rainfall over Bihar State, *India. Journal of Water and Land Development*. No. 36 p. 183–197. DOI: 10.2478/jwld-2018-0018

XLSTAT, (2018) Statistical software and data analysis add-on For Excel. Spectral analysis. retrieved from https://[www.xlstat.com/en/solutions/features/spectral-analysis](http://www.xlstat.com/en/solutions/features/spectral-analysis)

Zhao, X., Li, Z., Zhu, Q., Zhu, D., & Liu, H. (2017). Climatic and drought characteristics in the loess hilly-gully region of China from 1957 to 2014. PLoS One, 12(6), e0178701.

# APPENDIX I

**ANNUAL RAINFALL IN THE STUDY AREA**

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **2012** | **2011** | **1990** | **1989** | **1988** | **1987** | **1986** | **1985** | **1984** | **1983** | **1982** | **1981** | **1980** |
| 280 | 277 | 426 | 258 | 214 | 488 | 192 | 115 | 253 | 335 | 234 | 297 | 249 |
| 287 | 285 | 335 | 233 | 109 | 367 | 183 | 72 | 298 | 335 | 216 | 251 | 251 |
| 283 | 291 | 317 | 264 | 127 | 318 | 194 | 112 | 344 | 337 | 208 | 270 | 258 |
| 280 | 283 | 280 | 260 | 126 | 312 | 205 | 138 | 337 | 355 | 233 | 270 | 259 |
| 286 | 289 | 280 | 261 | 129 | 318 | 204 | 131 | 501 | 343 | 286 | 337 | 253 |
| 276 | 276 | 291 | 283 | 176 | 325 | 196 | 110 | 375 | 337 | 289 | 292 | 264 |
| 294 | 288 | 284 | 343 | 227 | 368 | 167 | 128 | 373 | 300 | 319 | 258 | 247 |
| 284 | 287 | 282 | 332 | 241 | 312 | 201 | 324 | 600 | 324 | 283 | 248 | 269 |
| 233 | 269 | 289 | 275 | 314 | 349 | 214 | 211 | 374 | 326 | 209 | 247 | 270 |
| 291 | 276 | 277 | 252 | 312 | 347 | 241 | 280 | 158 | 338 | 219 | 255 | 287 |
| 272 | 212 | 286 | 271 | 340 | 334 | 297 | 75 | 156 | 322 | 220 | 238 | 252 |
| 289 | 173 | 267 | 293 | 303 | 340 | 189 | 183 | 156 | 341 | 273 | 344 | 247 |
| 291 | 282 | 305 | 298 | 307 | 319 | 189 | 68 | 153 | 338 | 183 | 401 | 242 |
| 286 | 286 | 295 | 306 | 276 | 360 | 187 | 73 | 158 | 339 | 186 | 380 | 245 |
| 286 | 285 | 290 | 291 | 107 | 340 | 186 | 67 | 164 | 337 | 205 | 279 | 233 |
| 284 | 288 | 281 | 253 | 111 | 366 | 206 | 74 | 159 | 334 | 253 | 224 | 262 |
| 291 | 228 | 280 | 317 | 291 | 410 | 208 | 71 | 156 | 339 | 237 | 230 | 335 |
| 281 | 279 | 276 | 259 | 239 | 353 | 214 | 108 | 158 | 334 | 274 | 222 | 321 |
| 305 | 288 | 291 | 274 | 346 | 330 | 204 | 77 | 158 | 342 | 218 | 222 | 264 |
| 290 | 286 | 285 | 236 | 306 | 341 | 232 | 143 | 158 | 348 | 230 | 222 | 230 |
| 273 | 290 | 296 | 229 | 215 | 336 | 193 | 105 | 175 | 347 | 309 | 239 | 171 |
| 298 | 289 | 296 | 248 | 139 | 365 | 179 | 301 | 163 | 348 | 252 | 247 | 224 |
| 296 | 290 | 294 | 215 | 292 | 370 | 219 | 280 | 163 | 339 | 261 | 239 | 189 |
| 297 | 252 | 294 | 289 | 132 | 392 | 188 | 63 | 188 | 341 | 233 | 249 | 150 |
| 305 | 290 | 294 | 276 | 198 | 434 | 180 | 82 | 224 | 346 | 233 | 254 | 125 |
| 284 | 294 | 316 | 278 | 109 | 347 | 187 | 124 | 150 | 352 | 214 | 230 | 192 |
| 304 | 290 | 304 | 280 | 164 | 404 | 257 | 79 | 154 | 356 | 235 | 270 | 221 |
| 304 | 285 | 338 | 276 | 241 | 405 | 199 | 85 | 150 | 351 | 261 | 242 | 181 |
| 234 | 293 | 298 | 236 | 93 | 409 | 185 | 66 | 154 | 346 | 229 | 276 | 115 |
| 303 | 292 | 350 | 255 | 164 | 487 | 202 | 46 | 164 | 341 | 223 | 247 | 150 |
| 296 | 182 | 302 | 274 | 163 | 407 | 210 | 60 | 156 | 354 | 219 | 244 | 159 |
| 196 | 141 | 389 | 185 | 232 | 337 | 226 | 65 | 176 | 352 | 226 | 225 | 146 |
| 192 | 74 | 346 | 177 | 110 | 326 | 211 | 64 | 176 | 346 | 229 | 230 | 277 |
| 300 | 144 | 311 | 211 | 147 | 343 | 214 | 67 | 177 | 345 | 248 | 227 | 241 |

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 256 | 140 | 362 | 289 | 147 | 335 | 254 | 70 | 158 | 288 | 224 | 197 | 167 |
| 289 | 214 | 304 | 254 | 254 | 332 | 207 | 173 | 155 | 314 | 219 | 230 | 387 |
| 272 | 290 | 240 | 280 | 304 | 339 | 210 | 139 | 156 | 299 | 232 | 243 | 505 |
| 288 | 260 | 292 | 272 | 313 | 331 | 273 | 71 | 60 | 284 | 228 | 224 | 357 |
| 266 | 297 | 300 | 337 | 152 | 341 | 192 | 64 | 162 | 280 | 219 | 236 | 147 |
| 264 | 298 | 327 | 289 | 106 | 340 | 429 | 66 | 162 | 281 | 219 | 243 | 265 |
| 295 | 285 | 477 | 270 | 105 | 295 | 220 | 70 | 149 | 304 | 259 | 237 | 196 |
| 303 | 282 | 391 | 278 | 114 | 300 | 211 | 67 | 160 | 256 | 231 | 252 | 163 |
| 297 | 287 | 307 | 271 | 198 | 319 | 223 | 73 | 160 | 288 | 250 | 249 | 157 |
| 266 | 126 | 182 | 310 | 143 | 292 | 225 | 69 | 160 | 287 | 260 | 269 | 194 |
| 309 | 130 | 323 | 332 | 287 | 292 | 246 | 59 | 159 | 294 | 208 | 247 | 181 |
| 310 | 121 | 343 | 275 | 214 | 326 | 286 | 59 | 158 | 230 | 209 | 244 | 228 |
| 305 | 110 | 341 | 256 | 166 | 311 | 261 | 77 | 156 | 210 | 194 | 211 | 245 |
| 270 | 61 | 309 | 168 | 147 | 309 | 285 | 167 | 140 | 219 | 236 | 230 | 307 |
| 298 | 63 | 378 | 160 | 261 | 312 | 227 | 78 | 140 | 237 | 226 | 238 | 283 |
| 310 | 74 | 354 | 145 | 310 | 312 | 213 | 70 | 151 | 278 | 261 | 242 | 245 |
| 308 | 136 | 409 | 151 | 300 | 314 | 260 | 69 | 151 | 300 | 254 | 302 | 339 |
| 262 | 137 | 387 | 161 | 313 | 314 | 315 | 88 | 148 | 118 | 242 | 225 | 471 |
| 299 | 137 | 329 | 147 | 281 | 314 | 333 | 54 | 155 | 387 | 210 | 247 | 326 |
| 294 | 193 | 307 | 222 | 316 | 314 | 414 | 88 | 154 | 346 | 229 | 255 | 326 |
| 293 | 444 | 302 | 163 | 216 | 310 | 419 | 63 | 154 | 371 | 249 | 241 | 293 |
| 297 | 421 | 306 | 82 | 315 | 311 | 193 | 114 | 154 | 293 | 252 | 253 | 278 |
| 303 | 435 | 300 | 296 | 309 | 332 | 224 | 184 | 149 | 267 | 271 | 245 | 280 |
| 303 | 433 | 301 | 246 | 312 | 320 | 228 | 226 | 149 | 307 | 246 | 238 | 257 |
| 312 | 459 | 294 | 246 | 312 | 319 | 213 | 324 | 153 | 341 | 281 | 221 | 287 |
| 306 |  |  |  | 180 |  |  |  |  |  | 227 |  |  |
| 294 | 406 | 305 | 260 | 120 | 314 | 248 | 189 | 150 | 332 | 253 | 281 | 273 |
| 280 | 435 | 309 | 174 | 95 | 284 | 395 | 91 | 151 | 355 | 261 | 237 | 270 |
| 235 | 429 | 307 | 254 | 97 | 302 | 258 | 94 | 145 | 366 | 320 | 270 | 236 |
| 297 | 448 | 307 | 266 | 118 | 283 | 230 | 110 | 156 | 161 | 259 | 254 | 240 |
| 297 | 437 | 312 | 255 | 116 | 314 | 216 | 110 | 161 | 252 | 260 | 264 | 341 |
| 260 | 433 | 295 | 309 | 119 | 313 | 213 | 93 | 156 | 265 | 313 | 243 | 321 |
| 299 | 429 | 312 | 294 | 143 | 313 | 212 | 96 | 117 | 272 | 325 | 212 | 286 |
| 301 | 457 | 299 | 293 | 311 | 315 | 205 | 90 | 119 | 259 | 325 | 337 | 220 |
| 302 | 457 | 332 | 299 | 266 | 317 | 218 | 130 | 78 | 274 | 319 | 232 | 247 |
| 320 | 435 | 270 | 289 | 317 | 315 | 228 | 107 | 24 | 257 | 92 | 246 | 303 |
| 192 | 462 | 279 | 238 | 317 | 314 | 225 | 93 | 105 | 206 | 162 | 215 | 294 |
| 298 | 282 | 307 | 247 | 243 | 314 | 214 | 205 | 90 | 329 | 458 | 324 | 290 |
| 309 | 418 | 292 | 169 | 247 | 314 | 268 | 76 | 144 | 267 | 169 | 314 | 271 |
| 309 | 455 | 293 | 340 | 355 | 327 | 231 | 334 | 219 | 290 | 271 | 242 | 248 |

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 310 | 464 | 289 | 171 | 294 | 283 | 321 | 72 | 161 | 288 | 405 | 230 | 226 |
| 291 | 438 | 222 | 208 | 300 | 294 | 203 | 91 | 153 | 287 | 319 | 240 | 280 |
| 317 | 459 | 295 | 270 | 139 | 319 | 328 | 174 | 142 | 292 | 288 | 243 | 295 |
| 301 | 462 | 263 | 236 | 137 | 62 | 216 | 74 | 140 | 285 | 312 | 255 | 279 |
| 310 | 445 | 291 | 230 | 118 | 318 | 207 | 98 | 115 | 274 | 333 | 349 | 235 |
| 144 | 443 | 288 | 234 | 284 | 62 | 221 | 71 | 31 | 260 | 286 | 357 | 254 |
| 0 | 411 | 291 | 227 | 320 | 211 | 214 | 71 | 116 | 270 | 282 | 287 | 260 |
| 0 | 388 | 299 | 314 | 323 | 72 | 209 | 81 | 99 | 257 | 271 | 247 | 264 |
| 88 | 390 | 307 | 319 | 321 | 73 | 220 | 69 | 144 | 246 | 338 | 217 | 275 |
| 113 | 437 | 216 | 305 | 281 | 47 | 210 | 107 | 120 | 259 | 363 | 221 | 288 |
| 74 | 434 | 296 | 329 | 312 | 46 | 222 | 313 | 110 | 251 | 312 | 246 | 288 |
| 115 | 410 | 296 | 200 | 320 | 66 | 226 | 311 | 115 | 231 | 272 | 231 | 294 |
| 109 | 407 | 294 | 258 | 333 | 91 | 229 | 296 | 104 | 289 | 241 | 223 | 275 |
| 146 | 395 | 306 | 241 | 330 | 123 | 220 | 69 | 114 | 229 | 253 | 240 | 216 |
| 131 | 453 | 307 | 224 | 323 | 75 | 216 | 69 | 99 | 241 | 247 | 282 | 232 |
| 52 | 460 | 313 | 277 | 312 | 60 | 231 | 81 | 101 | 270 | 240 | 246 | 252 |
| 59 | 409 | 316 | 284 | 176 | 118 | 223 | 176 | 115 | 296 | 274 | 237 | 241 |
| 26 | 451 | 308 | 265 | 143 | 140 | 217 | 117 | 111 | 266 | 272 | 256 | 258 |
| 47 | 442 | 308 | 323 | 110 | 68 | 228 | 109 | 109 | 234 | 248 | 255 | 302 |
| 43 | 429 | 308 | 329 | 228 | 208 | 319 | 125 | 112 | 313 | 245 | 360 | 302 |
| 15 | 370 | 304 | 279 | 49 | 81 | 424 | 151 | 116 | 241 | 302 | 275 | 241 |
| 23 | 449 | 297 | 116 | 45 | 79 | 436 | 306 | 105 | 265 | 227 | 264 | 264 |
| 61 | 361 | 291 | 112 | 49 | 119 | 322 | 209 | 131 | 241 | 235 | 239 | 253 |
| 53 | 331 | 290 | 182 | 69 | 182 | 213 | 64 | 110 | 335 | 247 | 311 | 252 |
| 63 | 377 | 276 | 299 | 76 | 353 | 215 | 75 | 47 | 236 | 231 | 249 | 283 |
| 73 | 414 | 292 | 320 | 74 | 331 | 220 | 478 | 110 | 180 | 240 | 259 | 348 |
| 54 | 307 | 290 | 237 | 75 | 312 | 233 | 272 | 120 | 158 | 246 | 290 | 272 |
| 68 | 457 | 304 | 140 | 31 | 418 | 231 | 100 | 106 | 156 | 260 | 269 | 253 |
| 40 | 462 | 282 | 307 | 270 | 312 | 256 | 180 | 130 | 157 | 253 | 261 | 239 |
| 111 | 424 | 321 | 71 | 99 | 84 | 337 | 238 | 25 | 156 | 258 | 261 | 266 |
| 62 | 434 | 302 | 175 | 104 | 390 | 349 | 131 | 30 | 156 | 252 | 297 | 288 |
| 61 | 423 | 218 | 238 | 134 | 54 | 357 | 128 | 36 | 173 | 232 | 264 | 353 |
| 27 | 458 | 297 | 273 | 161 | 59 | 344 | 157 | 78 | 162 | 240 | 250 | 297 |
| 54 | 324 | 219 | 161 | 122 | 106 | 353 | 143 | 29 | 177 | 298 | 216 | 254 |
| 63 | 281 | 242 | 142 | 128 | 79 | 334 | 189 | 136 | 152 | 247 | 299 | 203 |
| 65 | 300 | 305 | 130 | 121 | 102 | 228 | 203 | 57 | 158 | 220 | 254 | 208 |
| 64 | 391 | 273 | 219 | 153 | 92 | 229 | 160 | 49 | 167 | 230 | 244 | 258 |
| 168 | 469 | 237 | 228 | 134 | 81 | 251 | 160 | 58 | 157 | 234 | 259 | 240 |
| 147 | 487 | 314 | 302 | 132 | 91 | 225 | 201 | 65 | 157 | 251 | 229 | 267 |
| 91 | 473 | 298 | 293 | 105 | 99 | 217 | 155 | 89 | 162 | 228 | 231 | 245 |

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 73 | 464 | 154 | 237 | 115 | 99 | 203 | 174 | 81 | 157 | 239 | 264 | 269 |
| 67 | 304 | 211 | 235 | 125 | 68 | 211 | 216 | 131 | 154 | 241 | 259 | 406 |
| 34 | 416 | 186 | 205 | 189 | 59 | 233 | 167 | 119 | 163 | 244 | 237 | 268 |
| 51 | 464 | 213 | 318 | 147 | 68 | 246 | 155 | 87 | 159 | 220 | 249 | 316 |
| 41 | 469 | 100 | 207 | 311 | 48 | 228 | 127 | 83 | 158 | 214 | 258 | 273 |
| 41 | 437 | 326 | 119 | 306 | 74 | 226 | 138 | 79 | 159 | 218 | 243 | 259 |
| 89 | 378 | 103 | 238 | 319 | 86 | 221 | 153 | 80 | 159 | 254 | 250 | 257 |
| 58 | 461 | 242 | 185 | 232 | 42 | 220 | 174 | 80 | 158 | 251 | 312 | 242 |
| 50 | 485 | 23 | 224 | 253 | 104 | 232 | 178 | 97 | 154 | 206 | 284 | 263 |
| 0 | 454 | 64 | 270 | 365 | 209 | 235 | 188 | 78 | 154 | 237 | 272 | 218 |
| 78 | 282 | 203 | 297 | 314 | 94 | 201 | 182 | 65 | 153 | 212 | 259 | 202 |
| 0 | 332 | 296 | 304 | 313 | 196 | 484 | 174 | 72 | 153 | 210 | 270 | 245 |
| 0 | 469 | 326 | 331 | 248 | 83 | 475 | 184 | 78 | 158 | 241 | 258 | 250 |
| 7 | 484 | 169 | 320 | 311 | 112 | 320 | 205 | 82 | 162 | 214 | 251 | 248 |
| 0 | 396 | 63 | 305 | 268 | 109 | 224 | 169 | 76 | 187 | 292 | 270 | 250 |
| 32 | 256 | 50 | 313 | 312 | 117 | 199 | 174 | 79 | 212 | 325 | 244 | 239 |
| 29 | 356 | 0 | 262 | 243 | 109 | 197 | 180 | 75 | 218 | 271 | 245 | 188 |
| 0 | 256 | 75 | 304 | 238 | 94 | 196 | 208 | 161 | 211 | 325 | 244 | 242 |
| 0 | 429 | 83 | 318 | 299 | 92 | 246 | 287 | 88 | 216 | 324 | 236 | 263 |
| 0 | 401 | 78 | 194 | 208 | 58 | 211 | 255 | 91 | 247 | 327 | 258 | 250 |
| 17 | 325 | 80 | 259 | 327 | 95 | 206 | 209 | 95 | 186 | 325 | 251 | 245 |
| 0 | 424 | 35 | 263 | 130 | 104 | 212 | 227 | 107 | 231 | 321 | 251 | 250 |
| 0 | 308 | 66 | 314 | 194 | 195 | 211 | 324 | 107 | 185 | 320 | 257 | 249 |
| 0 | 333 | 124 | 321 | 127 | 107 | 187 | 306 | 87 | 258 | 319 | 205 | 250 |
| 47 | 329 | 137 | 330 | 5 | 98 | 216 | 461 | 76 | 253 | 290 | 214 | 235 |
| 47 | 339 | 76 | 298 | 180 | 81 | 278 | 352 | 75 | 304 | 320 | 216 | 264 |
| 85 | 332 | 146 | 324 | 0 | 256 | 190 | 408 | 71 | 237 | 294 | 195 | 220 |
| 43 | 329 | 73 | 315 | 62 | 359 | 190 | 351 | 48 | 277 | 316 | 202 | 239 |
| 102 | 275 | 157 | 103 | 90 | 305 | 165 | 346 | 72 | 276 | 314 | 202 | 249 |
| 160 | 267 | 54 | 102 | 20 | 364 | 187 | 350 | 87 | 268 | 303 | 211 | 232 |
| 6 | 78 | 53 | 325 | 24 | 244 | 187 | 219 | 65 | 287 | 303 | 206 | 242 |
| 36 | 0 | 58 | 321 | 24 | 182 | 206 | 222 | 92 | 254 | 309 | 186 | 259 |
| 26 | 0 | 65 | 149 | 51 | 350 | 172 | 325 | 120 | 270 | 310 | 197 | 257 |
| 66 | 0 | 84 | 43 | 41 | 359 | 178 | 225 | 100 | 277 | 310 | 201 | 209 |
| 63 | 0 | 73 | 198 | 86 | 353 | 199 | 240 | 105 | 255 | 309 | 182 | 224 |
| 308 | 197 | 77 | 215 | 335 | 364 | 209 | 229 | 102 | 236 | 309 | 277 | 306 |
| 304 | 0 | 80 | 251 | 287 | 79 | 199 | 246 | 103 | 280 | 310 | 186 | 248 |
| 300 | 0 | 57 | 186 | 67 | 175 | 222 | 188 | 153 | 272 | 307 | 193 | 266 |
| 307 | 0 | 274 | 163 | 36 | 168 | 205 | 164 | 151 | 280 | 307 | 160 | 243 |

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 282 | 0 | 264 | 322 | 51 | 227 | 368 | 171 | 117 | 285 | 283 | 183 | 284 |
| 309 | 10 | 283 | 253 | 61 | 438 | 371 | 179 | 90 | 263 | 300 | 191 | 243 |
| 347 | 72 | 296 | 252 | 46 | 183 | 362 | 170 | 76 | 114 | 293 | 186 | 266 |
| 277 | 104 | 321 | 313 | 55 | 83 | 180 | 165 | 149 | 303 | 309 | 197 | 286 |
| 362 | 323 | 319 | 253 | 22 | 79 | 198 | 177 | 95 | 172 | 309 | 202 | 274 |
| 495 | 331 | 368 | 289 | 25 | 71 | 200 | 182 | 251 | 158 | 291 | 202 | 237 |
| 394 | 328 | 473 | 48 | 26 | 67 | 197 | 192 | 211 | 158 | 308 | 202 | 269 |
| 443 | 324 | 350 | 0 | 41 | 113 | 251 | 230 | 293 | 156 | 309 | 198 | 238 |
| 458 | 328 | 304 | 0 | 42 | 103 | 198 | 226 | 242 | 156 | 307 | 196 | 262 |
| 449 | 340 | 308 | 0 | 43 | 111 | 210 | 178 | 244 | 152 | 305 | 189 | 258 |
| 470 | 338 | 354 | 0 | 42 | 102 | 201 | 192 | 288 | 88 | 306 | 201 | 239 |
| 485 | 328 | 348 | 0 | 114 | 200 | 228 | 212 | 196 | 93 | 309 | 193 | 264 |
| 486 | 309 | 382 | 145 | 174 | 105 | 224 | 194 | 264 | 87 | 309 | 205 | 232 |
| 488 | 8 | 327 | 3 | 53 | 121 | 225 | 235 | 144 | 92 | 307 | 203 | 266 |
| 425 | 24 | 314 | 289 | 236 | 159 | 296 | 248 | 294 | 90 | 246 | 213 | 260 |
| 497 | 21 | 378 | 1 | 99 | 114 | 242 | 238 | 422 | 96 | 310 | 178 | 255 |
| 477 | 0 | 436 | 161 | 350 | 202 | 363 | 205 | 283 | 96 | 306 | 112 | 151 |
| 482 | 0 | 436 | 298 | 322 | 376 | 233 | 214 | 363 | 94 | 311 | 62 | 334 |
| 461 | 0 | 418 | 268 | 306 | 411 | 216 | 221 | 302 | 85 | 315 | 164 | 269 |
| 482 | 0 | 421 | 234 | 253 | 348 | 216 | 223 | 311 | 127 | 309 | 207 | 265 |
| 322 | 306 | 401 | 163 | 264 | 348 | 215 | 225 | 342 | 100 | 303 | 201 | 236 |
| 420 | 314 | 342 | 219 | 259 | 372 | 223 | 197 | 307 | 156 | 278 | 198 | 205 |
| 427 | 289 | 469 | 146 | 281 | 363 | 207 | 216 | 298 | 156 | 311 | 205 | 185 |
| 368 | 331 | 369 | 0 | 242 | 349 | 292 | 220 | 328 | 245 | 312 | 328 | 205 |
| 334 | 297 | 299 | 0 | 272 | 349 | 237 | 164 | 378 | 310 | 273 | 188 | 269 |
| 331 | 0 | 469 | 144 | 345 | 365 | 236 | 222 | 478 | 309 | 318 | 223 | 207 |
| 331 | 271 | 419 | 284 | 368 | 339 | 215 | 210 | 482 | 311 | 311 | 321 | 241 |
| 337 | 167 | 476 | 1 | 278 | 348 | 228 | 223 | 428 | 312 | 310 | 399 | 288 |
| 323 | 0 | 482 | 0 | 264 | 351 | 239 | 189 | 450 | 312 | 309 | 458 | 361 |
| 279 | 0 | 369 | 95 | 202 | 343 | 228 | 218 | 477 | 314 | 315 | 388 | 338 |
| 311 | 2 | 406 | 319 | 224 | 358 | 201 | 214 | 573 | 304 | 312 | 396 | 208 |
| 300 | 0 | 424 | 290 | 290 | 315 | 200 | 204 | 632 | 305 | 310 | 489 | 230 |
| 286 | 72 | 296 | 107 | 236 | 402 | 208 | 272 | 641 | 313 | 317 | 485 | 210 |
| 320 | 136 | 356 | 0 | 238 | 340 | 225 | 210 | 633 | 315 | 318 | 456 | 216 |
| 315 | 317 | 443 | 0 | 227 | 394 | 220 | 204 | 563 | 314 | 313 | 460 | 260 |
| 315 | 309 | 449 | 116 | 233 | 374 | 232 | 221 | 604 | 307 | 312 | 351 | 258 |
| 340 | 306 | 483 | 321 | 207 | 362 | 392 | 236 | 578 | 307 | 306 | 475 | 263 |
| 354 | 287 | 446 | 318 | 242 | 353 | 209 | 249 | 469 | 311 | 307 | 479 | 248 |
| 423 | 289 | 444 | 161 | 244 | 357 | 212 | 257 | 469 | 296 | 274 | 467 | 336 |
| 481 | 303 | 427 | 84 | 292 | 365 | 228 | 259 | 464 | 307 | 282 | 485 | 245 |

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 488 | 311 | 460 | 102 | 245 | 298 | 207 | 371 | 466 | 235 | 308 | 477 | 150 |
| 494 | 320 | 455 | 298 | 263 | 474 | 242 | 378 | 461 | 255 | 315 | 489 | 274 |
| 485 | 321 | 452 | 416 | 272 | 368 | 341 | 362 | 460 | 267 | 312 | 480 | 363 |
| 454 | 307 | 444 | 438 | 320 | 384 | 329 | 332 | 413 | 309 | 286 | 476 | 375 |
| 431 | 293 | 442 | 360 | 288 | 354 | 322 | 416 | 472 | 312 | 313 | 461 | 301 |
| 489 | 303 | 478 | 421 | 213 | 355 | 347 | 366 | 437 | 233 | 193 | 315 | 279 |
| 382 | 316 | 456 | 338 | 62 | 252 | 327 | 389 | 442 | 314 | 155 | 454 | 286 |
| 379 | 328 | 431 | 367 | 295 | 359 | 334 | 414 | 464 | 313 | 152 | 461 | 171 |
| 429 | 324 | 418 | 160 | 236 | 359 | 340 | 416 | 467 | 301 | 203 | 474 | 244 |
| 465 | 344 | 414 | 118 | 180 | 355 | 359 | 409 | 463 | 208 | 301 | 475 | 275 |
| 460 | 358 | 464 | 351 | 54 | 359 | 347 | 463 | 457 | 154 | 308 | 477 | 177 |
| 459 | 351 | 388 | 331 | 57 | 362 | 329 | 432 | 459 | 154 | 307 | 467 | 303 |
| 403 | 337 | 335 | 111 | 0 | 374 | 382 | 431 | 460 | 227 | 307 | 465 | 290 |
| 425 | 354 | 463 | 77 | 0 | 470 | 400 | 434 | 462 | 307 | 307 | 482 | 277 |
| 474 | 364 | 437 | 120 | 29 | 368 | 457 | 415 | 466 | 311 | 295 | 453 | 228 |
| 473 | 362 | 414 | 474 | 47 | 377 | 513 | 410 | 464 | 381 | 309 | 540 | 436 |
| 463 | 326 | 470 | 479 | 69 | 346 | 517 | 405 | 472 | 461 | 310 | 606 | 372 |
| 486 | 319 | 454 | 429 | 0 | 363 | 564 | 412 | 475 | 454 | 313 | 640 | 370 |
| 465 | 325 | 459 | 338 | 0 | 365 | 515 | 398 | 476 | 457 | 308 | 649 | 366 |
| 378 | 315 | 467 | 487 | 93 | 368 | 594 | 319 | 477 | 457 | 301 | 630 | 425 |
| 431 | 327 | 457 | 492 | 46 | 569 | 470 | 373 | 477 | 430 | 307 | 642 | 246 |
| 463 | 364 | 456 | 494 | 158 | 454 | 508 | 316 | 460 | 475 | 291 | 620 | 205 |
| 416 | 292 | 468 | 498 | 70 | 386 | 491 | 406 | 448 | 464 | 308 | 586 | 383 |
| 446 | 496 | 455 | 497 | 0 | 344 | 471 | 166 | 465 | 476 | 310 | 618 | 354 |
| 455 | 488 | 477 | 470 | 0 | 348 | 337 | 139 | 442 | 480 | 313 | 646 | 392 |
| 511 | 498 | 477 | 484 | 0 | 354 | 438 | 73 | 449 | 469 | 307 | 638 | 380 |
| 600 | 392 | 307 | 480 | 0 | 341 | 494 | 74 | 473 | 476 | 292 | 651 | 393 |
| 625 | 498 | 434 | 491 | 0 | 362 | 492 | 101 | 476 | 447 | 263 | 654 | 345 |
| 625 | 498 | 387 | 479 | 0 | 368 | 495 | 81 | 470 | 477 | 316 | 658 | 376 |
| 614 | 433 | 371 | 471 | 0 | 353 | 473 | 87 | 471 | 481 | 315 | 633 | 379 |
| 600 | 432 | 466 | 474 | 0 | 369 | 380 | 111 | 471 | 481 | 310 | 623 | 291 |
| 547 | 420 | 443 | 474 | 0 | 363 | 252 | 90 | 474 | 170 | 236 | 643 | 238 |
| 616 | 395 | 411 | 494 | 0 | 363 | 309 | 129 | 398 | 447 | 311 | 572 | 306 |
| 612 | 367 | 397 | 440 | 0 | 352 | 207 | 262 | 468 | 456 | 304 | 412 | 280 |
| 576 | 465 | 436 | 496 | 0 | 365 | 212 | 114 | 471 | 476 | 321 | 487 | 170 |
| 577 | 505 | 404 | 498 | 142 | 357 | 228 | 98 | 471 | 464 | 317 | 407 | 142 |
| 609 | 470 | 402 | 471 | 297 | 359 | 243 | 90 | 472 | 468 | 315 | 295 | 162 |
| 637 | 501 | 410 | 516 | 336 | 355 | 272 | 93 | 472 | 469 | 317 | 279 | 124 |
| 640 | 488 | 425 | 396 | 374 | 368 | 246 | 99 | 472 | 466 | 315 | 323 | 254 |
| 623 | 459 | 425 | 332 | 344 | 359 | 220 | 94 | 472 | 477 | 315 | 374 | 283 |

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 610 | 462 | 428 | 411 | 354 | 362 | 230 | 71 | 471 | 420 | 315 | 360 | 348 |
| 576 | 7 | 460 | 459 | 361 | 404 | 221 | 94 | 449 | 474 | 316 | 350 | 339 |
| 586 | 0 | 450 | 463 | 336 | 349 | 232 | 92 | 477 | 390 | 265 | 365 | 265 |
| 565 | 0 | 447 | 446 | 326 | 352 | 203 | 84 | 472 | 266 | 307 | 356 | 321 |
| 576 | 68 | 152 | 467 | 349 | 271 | 218 | 96 | 479 | 238 | 321 | 261 | 390 |
| 592 | 277 | 83 | 371 | 412 | 408 | 196 | 98 | 475 | 326 | 320 | 229 | 457 |
| 549 | 290 | 464 | 446 | 384 | 349 | 201 | 130 | 371 | 404 | 322 | 247 | 383 |
| 591 | 288 | 430 | 464 | 464 | 382 | 207 | 0 | 457 | 330 | 321 | 201 | 542 |
| 573 | 308 | 443 | 482 | 545 | 452 | 210 | 91 | 475 | 394 | 321 | 231 | 291 |
| 591 | 306 | 379 | 483 | 594 | 504 | 197 | 116 | 476 | 484 | 322 | 225 | 322 |
| 573 | 268 | 448 | 446 | 600 | 456 | 198 | 84 | 478 | 482 | 320 | 237 | 339 |
| 577 | 282 | 399 | 474 | 620 | 527 | 213 | 84 | 477 | 409 | 317 | 265 | 362 |
| 587 | 284 | 364 | 469 | 596 | 596 | 191 | 80 | 469 | 477 | 279 | 328 | 333 |
| 551 | 250 | 291 | 466 | 604 | 547 | 268 | 57 | 408 | 472 | 317 | 339 | 493 |
| 607 | 255 | 359 | 465 | 583 | 472 | 213 | 72 | 467 | 351 | 316 | 339 | 563 |
| 582 | 298 | 355 | 464 | 616 | 349 | 205 | 86 | 456 | 476 | 294 | 235 | 275 |
| 575 | 295 | 369 | 434 | 630 | 444 | 305 | 74 | 475 | 476 | 316 | 231 | 189 |
| 514 | 298 | 408 | 458 | 612 | 331 | 199 | 83 | 477 | 467 | 227 | 254 | 309 |
| 510 | 285 | 351 | 383 | 604 | 405 | 195 | 76 | 475 | 428 | 299 | 306 | 431 |
| 553 | 281 | 422 | 431 | 603 | 538 | 171 | 81 | 476 | 336 | 299 | 260 | 424 |
| 592 | 280 | 420 | 386 | 598 | 486 | 232 | 67 | 476 | 467 | 311 | 219 | 119 |
| 585 | 289 | 401 | 428 | 563 | 571 | 176 | 73 | 475 | 464 | 313 | 198 | 338 |
| 587 | 296 | 437 | 437 | 604 | 575 | 18 | 304 | 475 | 431 | 314 | 201 | 569 |
| 580 | 343 | 387 | 433 | 567 | 472 | 435 | 92 | 369 | 464 | 307 | 176 | 490 |
| 589 | 460 | 426 | 442 | 582 | 542 | 341 | 98 | 413 | 458 | 310 | 158 | 333 |
| 596 | 459 | 418 | 444 | 575 | 485 | 317 | 60 | 389 | 452 | 287 | 169 | 286 |
| 601 | 438 | 391 | 445 | 510 | 452 | 354 | 80 | 382 | 462 | 308 | 172 | 256 |
| 622 | 410 | 405 | 433 | 446 | 378 | 359 | 76 | 429 | 464 | 308 | 161 | 296 |
| 611 | 416 | 392 | 410 | 441 | 234 | 407 | 179 | 466 | 461 | 307 | 180 | 170 |
| 589 | 421 | 229 | 435 | 479 | 381 | 344 | 84 | 466 | 434 | 289 | 138 | 139 |
| 582 | 351 | 347 | 426 | 590 | 338 | 432 | 85 | 430 | 456 | 300 | 145 | 137 |
| 522 | 328 | 409 | 435 | 510 | 395 | 306 | 109 | 464 | 453 | 300 | 189 | 280 |
| 563 | 405 | 406 | 438 | 487 | 324 | 450 | 67 | 466 | 457 | 302 | 190 | 301 |
| 588 | 334 | 399 | 441 | 462 | 306 | 397 | 73 | 448 | 379 | 299 | 184 | 207 |
| 513 | 437 | 406 | 443 | 429 | 259 | 309 | 75 | 297 | 436 | 301 | 192 | 266 |
| 499 | 402 | 446 | 413 | 585 | 386 | 460 | 122 | 349 | 453 | 220 | 192 | 224 |
| 597 | 386 | 454 | 435 | 518 | 408 | 518 | 188 | 368 | 412 | 153 | 236 | 180 |
| 577 | 404 | 398 | 429 | 453 | 394 | 498 | 63 | 395 | 438 | 151 | 185 | 224 |
| 580 | 379 | 439 | 402 | 292 | 393 | 510 | 77 | 432 | 438 | 148 | 170 | 294 |
| 584 | 365 | 442 | 434 | 356 | 345 | 569 | 49 | 403 | 432 | 185 | 170 | 423 |

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 588 | 332 | 443 | 435 | 363 | 276 | 448 | 116 | 265 | 455 | 298 | 172 | 320 |
| 587 | 393 | 440 | 446 | 378 | 510 | 484 | 106 | 271 | 436 | 299 | 176 | 320 |
| 537 | 368 | 316 | 387 | 416 | 366 | 580 | 115 | 313 | 454 | 299 | 276 | 357 |
| 585 | 308 | 253 | 355 | 437 | 317 | 599 | 115 | 338 | 453 | 294 | 413 | 311 |
| 570 | 367 | 425 | 406 | 434 | 317 | 603 | 57 | 335 | 454 | 397 | 450 | 300 |
| 584 | 298 | 421 | 415 | 386 | 298 | 608 | 55 | 355 | 451 | 297 | 457 | 370 |
| 545 | 353 | 362 | 435 | 261 | 284 | 610 | 67 | 420 | 449 | 273 | 447 | 537 |
| 586 | 442 | 432 | 453 | 278 | 321 | 604 | 93 | 306 | 455 | 297 | 456 | 375 |
| 506 | 344 | 412 | 403 | 336 | 321 | 604 | 134 | 366 | 456 | 297 | 457 | 410 |
| 556 | 394 | 372 | 440 | 354 | 175 | 604 | 70 | 347 | 429 | 292 | 419 | 389 |
| 534 | 335 | 405 | 406 | 361 | 92 | 604 | 58 | 305 | 457 | 300 | 439 | 390 |
| 563 | 321 | 431 | 284 | 290 | 224 | 596 | 45 | 338 | 436 | 298 | 458 | 323 |
| 567 | 274 | 393 | 270 | 272 | 268 | 597 | 78 | 452 | 454 | 305 | 460 | 383 |
| 557 | 456 | 432 | 256 | 380 | 389 | 588 | 77 | 424 | 448 | 306 | 458 | 437 |
| 554 | 432 | 449 | 266 | 484 | 353 | 595 | 78 | 454 | 368 | 305 | 408 | 456 |
| 541 | 431 | 414 | 286 | 447 | 366 | 600 | 39 | 370 | 363 | 301 | 449 | 610 |
| 576 | 349 | 443 | 288 | 421 | 330 | 600 | 73 | 454 | 350 | 300 | 420 | 612 |
| 530 | 440 | 444 | 432 | 502 | 333 | 599 | 64 | 326 | 373 | 262 | 435 | 606 |
| 453 | 439 | 416 | 443 | 367 | 339 | 591 | 61 | 418 | 437 | 287 | 436 | 609 |
| 460 | 445 | 222 | 432 | 393 | 316 | 579 | 84 | 452 | 451 | 302 | 380 | 549 |
| 577 | 437 | 0 | 420 | 452 | 312 | 589 | 64 | 425 | 428 | 297 | 313 | 616 |
| 577 | 438 | 0 | 436 | 382 | 423 | 595 | 153 | 348 | 383 | 299 | 307 | 617 |
| 567 | 311 | 0 | 438 | 324 | 332 | 592 | 55 | 361 | 364 | 299 | 307 | 616 |
| 504 | 349 | 0 | 442 | 434 | 331 | 584 | 64 | 343 | 336 | 303 | 296 | 614 |
| 422 | 339 | 0 | 344 | 411 | 337 | 597 | 89 | 430 | 299 | 303 | 318 | 613 |
| 541 | 331 | 0 | 295 | 307 | 318 | 530 | 94 | 430 | 303 | 199 | 318 | 606 |
| 560 | 353 | 0 | 292 | 300 | 319 | 542 | 103 | 453 | 305 | 168 | 456 | 602 |
| 477 | 343 | 0 | 291 | 311 | 328 | 499 | 114 | 453 | 384 | 251 | 443 | 613 |
| 441 | 347 | 89 | 291 | 323 | 339 | 564 | 108 | 390 | 474 | 300 | 457 | 523 |
| 565 | 355 | 265 | 289 | 330 | 337 | 473 | 139 | 372 | 327 | 300 | 373 | 585 |
| 581 | 301 | 286 | 289 | 360 | 327 | 476 | 124 | 338 | 308 | 251 | 303 | 620 |
| 315 | 410 | 292 | 293 | 325 | 338 | 547 | 101 | 307 | 305 | 237 | 215 | 610 |
| 424 | 420 | 294 | 289 | 329 | 351 | 594 | 65 | 303 | 339 | 302 | 280 | 608 |
| 350 | 309 | 290 | 291 | 288 | 337 | 581 | 80 | 338 | 301 | 300 | 305 | 537 |
| 436 | 326 | 288 | 292 | 366 | 284 | 524 | 82 | 379 | 312 | 249 | 307 | 471 |
| 434 | 278 | 286 | 287 | 360 | 351 | 554 | 82 | 293 | 281 | 294 | 224 | 423 |
| 417 | 275 | 284 | 264 | 330 | 335 | 466 | 104 | 318 | 299 | 303 | 229 | 371 |
| 386 | 268 | 285 | 291 | 264 | 334 | 511 | 88 | 296 | 238 | 302 | 257 | 303 |

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 416 | 278 | 289 | 288 | 227 | 320 | 437 | 95 | 302 | 260 | 301 | 287 | 253 |
| 317 | 275 | 187 | 288 | 235 | 321 | 483 | 134 | 297 | 254 | 301 | 300 | 226 |
| 325 | 274 | 201 | 294 | 253 | 317 | 420 | 83 | 414 | 349 | 302 | 286 | 285 |
| 399 | 272 | 97 | 288 | 254 | 320 | 505 | 160 | 455 | 514 | 300 | 267 | 248 |
| 432 | 188 | 131 | 294 | 296 | 310 | 421 | 164 | 438 | 610 | 302 | 251 | 245 |
| 320 | 291 | 292 | 255 | 302 | 310 | 361 | 88 | 303 | 601 | 303 | 237 | 270 |
| 281 | 278 | 279 | 291 | 441 | 321 | 441 | 90 | 400 | 610 | 282 | 208 | 237 |
| 320 | 263 | 280 | 284 | 321 | 326 | 436 | 161 | 315 | 616 | 304 | 240 | 298 |
| 284 | 274 | 277 | 282 | 236 | 345 | 433 | 188 | 305 | 612 | 303 | 226 | 260 |
| 278 | 260 | 294 | 356 | 341 | 334 | 431 | 181 | 337 | 618 | 303 | 221 | 256 |
| 305 | 261 | 286 | 427 | 355 | 341 | 380 | 202 | 261 | 618 | 303 | 252 | 291 |
| 305 | 283 | 281 | 425 | 302 | 347 | 306 | 199 | 331 | 454 | 303 | 228 | 252 |
| 291 | 280 | 292 | 376 | 261 | 336 | 434 | 196 | 298 | 613 | 303 | 226 | 233 |
| 270 | 267 | 283 | 389 | 331 | 340 | 318 | 79 | 300 | 617 | 304 | 226 | 253 |
| 205 | 293 | 269 | 422 | 291 | 339 | 331 | 196 | 299 | 616 | 304 | 228 | 251 |
| 366 | 290 | 286 | 396 | 202 | 32 | 313 | 188 | 297 | 618 | 304 | 227 | 325 |
| 316 | 294 | 253 | 355 | 213 | 318 | 329 | 191 | 355 | 586 | 301 | 231 | 315 |
| 282 | 290 | 298 | 289 | 158 | 329 | 318 | 209 | 306 | 619 | 301 | 272 | 313 |
| 310 | 282 | 295 | 276 | 268 | 334 | 310 | 195 | 304 | 625 | 304 | 251 | 327 |
| 396 | 294 | 296 | 293 | 235 | 299 | 326 | 173 | 305 | 612 | 304 | 238 | 260 |
| 336 | 292 | 278 | 294 | 232 | 296 | 315 | 193 | 306 | 579 | 304 | 235 | 285 |
| 346 | 290 | 287 | 294 | 238 | 305 | 206 | 193 | 307 | 534 | 301 | 197 | 312 |
| 218 | 298 | 282 | 288 | 189 | 284 | 88 | 209 | 304 | 621 | 301 | 140 | 257 |
| 436 | 289 | 299 | 297 | 273 | 238 | 91 | 202 | 301 | 625 | 303 | 207 | 267 |
| 318 | 277 | 284 | 328 | 228 | 237 | 133 | 191 | 306 | 595 | 300 | 210 | 226 |
| 279 | 312 | 291 | 376 | 221 | 227 | 239 | 199 | 250 | 499 | 111 | 212 | 230 |
| 270 | 294 | 286 | 331 | 189 | 232 | 410 | 241 | 372 | 580 | 298 | 214 | 224 |
| 312 | 295 | 280 | 335 | 291 | 221 | 146 | 249 | 308 | 564 | 304 | 207 | 248 |
| 333 | 295 | 272 | 329 | 332 | 229 | 282 | 200 | 307 | 581 | 306 | 228 | 353 |
| 367 | 300 | 270 | 326 | 371 | 243 | 124 | 203 | 304 | 454 | 308 | 226 | 322 |
| 366 | 300 | 276 | 314 | 294 | 232 | 330 | 190 | 302 | 402 | 308 | 222 | 259 |
| 421 | 302 | 268 | 262 | 328 | 230 | 329 | 187 | 310 | 394 | 307 | 243 | 277 |
| 430 | 302 | 289 | 286 | 290 | 223 | 333 | 186 | 293 | 461 | 306 | 216 | 254 |
| 429 | 304 | 292 | 289 | 136 | 248 | 334 | 136 | 353 | 437 | 306 | 215 | 257 |
| 435 | 102 | 297 | 291 | 325 | 223 | 322 | 162 | 294 | 446 | 208 | 202 | 193 |
| 418 | 279 | 288 | 279 | 203 | 225 | 318 | 141 | 93 | 415 | 151 | 200 | 369 |
| 331 | 306 | 209 | 328 | 225 | 234 | 327 | 188 | 289 | 402 | 147 | 210 | 230 |
| 562 | 296 | 275 | 334 | 240 | 133 | 317 | 192 | 361 | 418 | 153 | 205 | 239 |
| 366 | 293 | 287 | 353 | 255 | 117 | 286 | 196 | 350 | 444 | 154 | 203 | 231 |
| 304 | 287 | 289 | 316 | 300 | 129 | 319 | 205 | 304 | 428 | 153 | 212 | 265 |

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 265 | 284 | 288 | 362 | 297 | 235 | 317 | 178 | 252 | 442 | 153 | 204 | 263 |
| 295 | 290 | 237 | 321 | 288 | 288 | 316 | 160 | 299 | 471 | 218 | 224 | 247 |
| 304 | 294 | 289 | 323 | 297 | 228 | 320 | 203 | 294 | 430 | 376 | 214 | 247 |
| 275 | 295 | 296 | 292 | 230 | 142 | 320 | 220 | 319 | 453 | 352 | 269 | 213 |
| 466 | 299 | 364 | 280 | 231 | 229 | 318 | 207 | 350 | 505 | 305 | 182 | 339 |
| 362 | 285 | 284 | 317 | 221 | 103 | 323 | 197 | 370 | 401 | 304 | 303 | 327 |
| 295 | 273 | 244 | 341 | 250 | 105 | 324 | 199 | 261 | 316 | 306 | 240 | 259 |
| 363 | 334 | 292 | 292 | 235 | 101 | 326 | 207 | 241 | 284 | 336 | 228 | 354 |
| 313 | 358 | 296 | 321 | 237 | 213 | 325 | 202 | 183 | 385 | 440 | 273 | 287 |
| 296 | 319 | 284 | 306 | 220 | 223 | 302 | 209 | 153 | 414 | 410 | 226 | 264 |
| 303 | 295 | 105 | 298 | 238 | 119 | 328 | 178 | 151 | 565 | 307 | 287 | 274 |
| 426 | 297 | 221 | 300 | 243 | 237 | 330 | 180 | 193 | 397 | 368 | 212 | 272 |
| 278 | 297 | 206 | 256 | 238 | 123 | 334 | 198 | 305 | 325 | 365 | 208 | 271 |
| 283 | 274 | 275 | 301 | 244 | 110 | 352 | 184 | 268 | 287 | 373 | 229 | 275 |
| 289 | 285 | 284 | 237 | 248 | 208 | 565 | 183 | 271 | 317 | 366 | 220 | 302 |